{"text_format":"3","workbook":"xls","n_sheets":2,"sheets":["设备清单","Sheet1"],"not_rendered":{"charts":1,"images":14,"external_links":1,"defined_names":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"设备清单","index":0,"n_rows":18,"n_cols":12,"rows_kept":18,"merged":[[0,0,0,11],[2,0,2,11],[17,1,17,8]],"flags":["formulas_cached_only"]}
["www.pro001.com 陈先生 18501635951"]
["序号","设备名称","品牌","型号","技术参数","国别","单位","数量","单价","小计","类似图样","备注"]
["一、礼堂扩声系统"]
[1,"返听","YY  audio","MR15","MR15是一款15\"同轴两分音全音域监听音箱。采用一只15\"高效率同轴单元，90°恒指向性号角，箱体采用多层复合夹板，特殊喷涂制作。\n\n●高质量单元配置，高强度夹板箱体\n●多角度设计适合不同舞台\n●超长品质保证期：品质与信心的保证\n\n●多功能厅、高级酒店会所 \n●流动商演、乐队扩声以及舞台返送音箱","中国","只",2]
[2,"线阵","YY  audio","LA5312","LA5312是一款远射程、高精度线性阵列扬声器系统，它具有极大的动态容量，组件上的相位校正以及专利线性号角应用能完美的重放规定范围内频谱信号。吊挂系统采用最新人性化设计，使整个系统安装快捷、安全。单元配置：一只12\"高效率低音单元，两只5\"强磁中音单元，两只1\"×6\"声透镜配置两只1\"喉口44芯强磁高音驱动器，箱体采用多层复合夹板，特殊喷涂制作。\n\n●高质量单元配置，专利线性号角：音质优美，投射精确\n●真正三分音设计，内、外置分频选择：  使操作简便灵活\n●方便简捷的吊挂方式：安装简易快捷\n●超长品质保证期：品质与信心的保证\n\n●体育场馆、大型演出系统\n●剧院、音乐厅、演艺中心、会议中心","中国","只",8]
[3,"线阵低音","YY  audio","LA118B","频率响应   40Hz-300Hz\n单元组成   1×18\"(460mm)/4\"voice coil LF\n额定功率   600W RMS,2400W peak\n灵敏度   99dB 1watt/1 metre\n声压级   127 dB continuous,133 dB peak\n额定阻抗   8 ohms nominal\n输入方式   2×Speakon NL4\n包装尺寸   775mm×860mm×775mm(Flight case/pc) 895mm×795mm×615mm\n净重   71.5 kg/pc\n毛重   108.5kg/(Flight case/pc) 77.5 kg/pc","中国","只",2]
[4,"功放","YY  audio","MA1100","立体声功率 8Ω:\t2×550W\n立体声功率 4Ω:\t2×840W\n桥接功率 8Ω:      1680W\n信噪比\t ≥98dB\n转换率:\t 15V/μS\n阻尼系数:\t >230 Nominal operating condition 1KHz/8Ω\n频响:\t ±1dB Nominal operating condition 20Hz-20KHz\n总谐波失声:\t ≤0.03% Nominal operating condition 1kHz/8Ω\n互调失声:\t \t≤0.1Nominal operating condition 60Hz/7kHz 4:1\n\n输入灵敏度\t \t0.77V\n\n输入阻抗\t \t20kΩ/Balancde,10kΩ/un-Balanced\n\n分离度\t \t62dB Rated Out 1kHz/8Ω\n\nLED指示\t \tProtect,Clip,Signal,Bridge,Stereo,Parallel,Power\n\n保护功能\t \tSoft Start,Short Circuit,Limiter,DC Fault,AC Line Fuse,Thermal Cut\n\n散热系统\t \tTwo steps speed fan\n\n电源\t \tAC:220-230V 50Hz/60Hz\n\n重量\t \t17Kg\n\n尺寸\t \t482x460.5×88 mm","中国","台",5]
[5,"低音功放","YY  audio","MA2600","立体声功率 8Ω:\t 2×1300W\n立体声功率 4Ω:\t 2×1820W\n桥接功率 8Ω:\t 3600W\n信噪比\t ≥98dB\n转换率:\t 15V/μS\n阻尼系数:\t >230 Nominal operating condition 1KHz/8Ω\n频响:\t ±1dB Nominal operating condition 20Hz-20KHz\n总谐波失声:\t≤0.03% Nominal operating condition 1kHz/8Ω\n互调失声:\t \t≤0.1Nominal operating condition 60Hz/7kHz 4:1\n输入灵敏度\t 0.77V\n输入阻抗\t \t20kΩ/Balancde,10kΩ/un-Balanced\n分离度\t \t62dB Rated Out 1kHz/8Ω\nLED指示\t \tProtect,Clip,Signal,Bridge,Stereo,Parallel,Power\n\n保护功能\t \tSoft Start,Short Circuit,Limiter,DC Fault,AC Line Fuse,Thermal Cut\n\n散热系统\t \tTwo steps speed fan\n\n电源\t \tAC:220-230V 50Hz/60Hz\n\n重量\t \t34Kg\n\n尺寸\t \t482x460.5×132mm","中国","台",1]
[6,"吊麦","SHURE","MX202B/C","产品类型\t有线\t收音头\t电容式\n指向特征\t心形指向\t频响范围\t50Hz-17kHz\t \t \n灵敏度\t-35.0 dBV/Pa\n频响范围\t 50Hz-17kHz\t阻抗\t180 Ω\n信噪比\t 66.0 dB\t \t ","美国","只",6]
[7,"鼓话筒","SHURE","BETA57A","优质的话筒，为配合扩音乐器或非电声乐器使用而设计,紧凑的网罩设计可以使话筒头接近声源","美国","只",3]
[null,"乐器话筒","SHURE","BETA98H/C","心形电容话筒，配有灵活的鹅颈配件，可直接夹在号口或鼓沿处，易于精确定位。可用于：弦乐器/铜管乐器/木管乐器/萨克斯风，20HZ-20KHZ，超心形指向性。","美国","只",3]
[8,"手持话筒","SHURE","BLX-288/SM58","技术规格\n\n每个频段可兼容的系统数量: 12\n自动设置功能: 频道/组扫描\n音频参考压缩扩展: 是\n天线: 1/4波长天线\n天线选项: 是\nPC控制: 否\n机架部件: 已包含\n外壳: 模塑ABS，钢质\n接收机显示屏: 多功能LCD + LED\n电池，供电时间: 碱性电池：14小时\n环境: KTV，酒吧，会议中心，酒店，教堂，学校","美国","只",4]
[null,"领夹话筒","SHURE","SLX14/93","SLX无线领夹式系统，包括 WL93 全向微型领夹式话筒、SLX1 腰包式发射机和 SLX4 分集接收机","美国","只",4]
[9,"大震膜有线话筒","AKG","C4000B","指向性：可在心型、超心型及全指向之间进行切换。\n　　* 频响范围：20-20,000Hz。\n　　* 灵敏度：25 mV/Pa (-32 dBV)。\n　　* 最大声压级：145/155 dB (THD=0.5%)。\n　　* 等效噪声电平（CCIR 468-3）：19dB。\n　　* 等效噪声电平：8 dB-A。\n　　* 信/噪比：86 dB。\n　　* 低频衰减：-10 dB，带开关。\n　　* 低切滤波器：12 dB/倍频程 100 Hz。\n　　* 阻抗：200Ω。\n　　* 推荐负载阻抗：>1.000Ω。\n　　* 供电电压：9 - 52 V 幻像供电至DIN 45596。\n　　* 电流消耗：<2 mA。\n　　* 连线插口：3针XLR。\n　　* 外观颜色：银灰色。\n　　* 尺寸：58 直径 x 183 毫米。\n　　* 净重：450克。\n　　* 运输重量：1千克。\n　　* 附件：H100防震架，W4000防风罩。  \n","奥地利","只",4]
[10,"效果器","TC","M.ONEXL","立体声数字混响效果器,双处理器(输入输出采用XLS平衡插头)","丹麦","台",1]
[null,"声卡","ROLAND","UA55","两个配有专业话筒前级放大器的XLR/TRS输入接口，两个TRS输出接口，一个同轴I/O接口，一个耳机输出接口和一个MIDI I/O接口\n图示化控制面板软件带给您对话筒前级放大器迅速直观的控制\n幻象电源，Ground Lift，高抗阻（Hi-Z）开关\n一键AUTO-SENS功能将把您的话筒前级放大器智能地设置为最佳输入电平\n超低延迟VS Streaming驱动\n低噪、宽频电力供应\n持久耐用的铝质机身与Direct Box功能的紧密结合","日本","台",1]
[null,"均衡器","ASHLY","GQX3102"," 阻尼式金属轴臂推子\n• 低失真、高精度的 Wein- 桥式滤波器\n• \"Q\" 值恒定，\"平直\"位处保持低波纹系数和精确响应\n• 平衡式 XLR、1/4\" 立体声直插和端子接头式输入\n• 准平衡式 XLR、1/4\" 立体声直插和端子接头式输出\n• 31 段均衡器型号具有可选 15dB 或 6dB 范围\n• 31 段均衡器型号具有开关可调式高通滤波器\n• 31 段均衡器型号具 10 位、2 色 LED 电平表及峰值 LED 显示器\n\n","美国","台",1]
[null,"合计",{"$nulls":7},0]

{"sheet":"Sheet1","index":1,"n_rows":27,"n_cols":8,"rows_kept":27,"merged":[[0,0,0,10],[3,2,3,5],[4,2,4,5],[5,2,5,5],[6,2,6,5],[7,2,7,5],[8,2,8,5],[9,2,9,5],[10,2,10,5],[11,2,11,5],[12,0,12,1],[12,2,12,4],[13,0,13,1],[13,2,13,4],[14,0,14,10],[15,0,15,10],[16,0,16,10],[17,0,17,10],[18,0,18,10],[19,0,19,10],[20,5,20,8],[22,5,22,7]],"flags":["formulas_cached_only"]}
["山东省五莲县实验学校礼堂音响系统"]
["呈送","王总",{"$nulls":5},"日期：2014.5.15"]
["计划","上海雍阳电子科技有限公司",{"$nulls":3},"联系人：耿以才   15221297216"]
["NO.","ENGINEERING ITEM","AMOUNT"]
["序号","工 程 项 目","金 额"]
["一","设备总计",{"v":0,"d":"￥0.00"}]
["二","以上设备总计",{"v":0,"d":"￥0.00"}]
["三","安装调试费15%",{"v":0,"d":"￥0.00"}]
["四","设计费3%",{"v":0,"d":"￥0.00"}]
["五","差旅费3%",{"v":0,"d":"￥0.00"}]
["六","增值税9%",{"v":0,"d":"￥0.00"}]
["七","以上合计",{"v":0,"d":"￥0.00"}]
["TOTAL（RMB）",null,{"v":0,"d":"￥0.00"},null,null,"圆整"]
["累计金额（人民币）",null,0,null,null,"圆整"]
["承诺：本公司所售设备为100%正品行货，三包齐全。客户收到货后如与合同要求的型号规格不同或非原装正品，可以立即无条件退货，来回运费由乙方承担"]
["一、付款方式：合同签订后付定金30%，（即付人民币：元），发货前付合同总额的60%（即付人民币：元），安装调试完成附合同总额的10% （即付人民币：元）。（安装调试完毕，七天内付清全款，每逾期一天按合同总额的1%作为逾期金补偿给乙方。"]
["二、质保：质保期1年，质保期内甲方只要付来回运费即可，其余零配件费用由乙方负责，终身维护，质保期之后乙方只收取零配件成本费，来回运费由甲方承担。"]
["三、货期：付定金后7天内发货（ 付全款后第二天发货），运输时间为3-4天。（安装调试时间：3-7天。）\n发货点：本公司物流仓库有三个点：广东，上海，河北，大部分主设备由广东发出，进口商品多数由上海发出，河北仓库负责北方地区的部分物流。\n                                                                                          "]
["四、安装调试：乙方只负责供货"]
["五、收货地址：            收货人：                  联系电话："]
["甲方：",{"$nulls":4},"乙方：上海雍阳电子科技有限公司"]
["联系电话：",{"$nulls":4},"联系电话：15221297216"]
["联系人：",{"$nulls":4},"联系人：耿以才"]
["法人或受权人签字盖章：",{"$nulls":4},"法人或受权人签字盖章："]
["日期   年    月   日",{"$nulls":4},"日期：2014 年 5 月 15 日"]
[]
["此报价3天内有效，3天后另行报价。"]