{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["私人会所--100平以内"],"not_rendered":{"images":8},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"私人会所--100平以内","index":0,"n_rows":17,"n_cols":10,"rows_kept":17,"merged":[[0,0,0,9],[16,0,16,8]],"flags":["formulas_cached_only"]}
["北京某私人会所音响配置"]
["序号","设备名称 ","品牌","型号","产品参数","原产地","数量","单位","单价","小计"]
["A、扬声器系统"]
["A1","主扩扬声器","L-ACOUSTICS","12XTi","可用带宽：55Hz--20kHz（-10dB）\n角度：水平:90° 垂直：90°\n最大声压级：133dB\n单元：低音：12寸  高音：3寸\n功率：被动分频模式：380瓦， 主动模式：低音 290瓦 高音135瓦\n尺寸（高x宽x深）：540 x 410 x 389 mm；\n重量：29千克；","法国",4,"只"]
["A2","主扩扬声器吊挂件","L-ACOUSTICS","ETR12XTi","12XTi扬声器安装支架，可调角度","法国",4,"套"]
["A3","单18吋超低频扬声器","L-ACOUSTICS","SB18i","可用带宽：32Hz-100Hz（-10dB）\n指向性：360°\n最大声压级：136dB\n单元：低音：1*18寸\n功率：700瓦在8Ω\n尺寸（高x宽x深）：538 x 754 x 717 mm\n重量：62千克","法国",2,"只"]
["B、音频数字处理及功率放大器系统"]
["B1","四通道数字网络音频处理功放","L-ACOUSTICS","LA4x","4通道数字信号处理及功率放大器系统\n24Bit AD/DA，96KHz，32Bit内部运算；增益、压限、延时、均衡、分频、矩阵；计算机远程监控系统，以太网络接口(RJ45)\n4 路平衡模拟输入/输出(XLR)\n4×4数字处理路由矩阵\n4通道功率放大器\n内置AES/EBU数字接口扩展卡\nRMS功率：4×1000W/8Ω，4×1000W/4Ω","法国",2,"台"]
["C2","数字功放远程控制管理软件","L-ACOUSTICS","L-NET",null,"法国",1,"套"]
["C、无线话筒"]
["C1","真集式双通道无线话筒接收机","Sennheiser","EM 2050","真集式双通道无线话筒接收机；\nUHF内5个频率区间，最大可达75MHz的频宽；\n通过网线直接用电脑监控；\n自带天线分配器，最多可8台共用天线；\n内建频率均衡器；","德国",1,"台"]
["C2","手持话筒无线发射器","Sennheiser","SKM 2000","最高可达到75MHz的交换频宽；\n20个固定频带，最多64个可兼容的预设；\n6组每组最多64个可调谐的通道；\n频率设置以25kHz为步长；\n外部充电触点让你可以直接给话筒内的BA 2015电池充电；\n音频和射频静音功能；\n可以通过红外传输与接收机同步；","德国",2,"支"]
["C3","超心形话筒头","Sennheiser","MMD 945","超心形动圈话筒头","德国",2,"个"]
["D、吸定扬声器"]
["D1","定压吸顶扬声器","KDLK","IC-105T","5”（130mm）玻纤低音和反相铝质圆顶高音","法国",10,"个"]
["D2","专业功放","KDLK",2120,"2*120W","法国",1,"台"]
["总计：",{"$nulls":8},{"v":0,"d":"0.00"}]