{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["铜仁酒吧"],"not_rendered":{"images":28},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"铜仁酒吧","index":0,"n_rows":47,"n_cols":11,"rows_kept":47,"merged":[[0,0,0,9],[34,0,34,8]],"flags":["formulas_cached_only"]}
["贵州铜仁酒吧(约500平方）"]
["序号","设备名称","品牌、型号","技术参数","国别","单位","数量","单价","小计","类似图样","备注"]
["一、音响及功放部分"]
[1,"主音箱","YYAUDIO YA15","频率响应范围：40HZ-18HZ；单元组成：1X15\"(385mm)/3\"1X1.4\"(36mm)/1.7；额定功率：400W RMS,1600Wpeak；灵敏度：98db/1watt/1metre；声压级：124db continuous;130db peak;额定阻抗：8 ohms nominal;","中国","只",2]
[2,"音箱","YY audio YA12","频率响应范围：50HZ-18HZ；单元组成：1X12\"(300mm)3\"1X1\"(25mm)1.7；额定功率：300W RMS,1200Wpeak；灵敏度：97db/1watt/1metre；声压级：122db continuous;128db peak;额定阻抗：8 ohms nominal;","中国","只",6]
[3,"超低音音箱","YA118B","频率响应范围：40HZ-150HZ；单元组成：1X18\"(460mm)/4；额定功率：600W RMS,2400Wpeak；灵敏度：100db/1watt/1metre；声压级：128db continuous;134db peak;额定阻抗：8 ohms nominal;","中国","只",2]
[4,"返听音响","YA10","频率响应范围：55HZ-20HZ；单元组成：1X10\"(250mm)2.5\"1x1\"(25mm)；额定功率：250W RMS,1000Wpeak；灵敏度：95db/1watt/1metre；声压级：119db continuous;125db peak;额定阻抗：8 ohms nominal;","中国","只",2]
[5,"主功放","UA1200","■Channel 2■2频道■8Ω Stereo Power 600W■8Ω立体声功率600■4Ω Stereo Power 900W■4Ω立体声功率900■2Ω Stereo Power 1100W■2Ω立体声功率1100■8Ω Bridged Power 1800W■8Ω桥接功率1800■4Ω Bridged Power 2000W■4Ω桥接功率2000■Signal to Noise >105dB■信号噪声> 105dB■Slew Rate >80V/us■摆率> 80V /美国■Damping Factor >500■阻尼系数> 500■Frequency Response (+/-0.1dB)■频率响应（+ / - 0.1dB）20Hz+20KHzz 20kHz +■THD (Rated power@ 8 Ohm, 1KHz) <0.01%■THD（额定电源8欧姆，1kHz）＜0.01%■LMD(Rated power@ 8 Ohm) <0.01%■LMD（额定电源8欧姆）＜0.01%■Input Sensitivity 0.775V,1.0V,1.55V■输入灵敏度0.775V，1.0V 1.55V■Input Impedance 10K Ohm Unbalanced;■10K欧姆不平衡输入阻抗；20K Ohm Balanced20K欧姆平衡■LPF 20Hz-180Hz Valid■LPF 20hz-180hz有效■HPF 130Hz-20KHz Valid■HPF 130hz-20khz有效■Input CMRR <-75dB■输入共模抑制比< 75dB■Cross Talk <-70dB■相声＜70分贝■Main Power Supply 220V 50/60Hz,■主电源220V 50或60Hz，Fuse:T12A保险丝：T12A■Protection Short Circuit, Overload,■保护短路，过载，Overvoltage, Overheat过压，过热■Size W*D*H(cm) 48.3*49*88■大小W * D * H（48.3×49×88厘米）■N.W. 22 kg■净重22公斤■Unit Piece■元块","中国","台",1]
[6,"环绕功放，返听功放","UA800","■2频道\n■8Ω Stereo Power 400W\n■8Ω立体声功率400\n■4Ω Stereo Power 600W\n■4Ω立体声功率600\n■2Ω Stereo Power 800W\n■2Ω立体声功率800\n■8Ω Bridged Power 1000W\n■8Ω桥接功率1000\n■4Ω Bridged Power 1200W\n■4Ω桥接功率1200\n■Signal to Noise >105dB\n■信号噪声> 105dB\n■Slew Rate >60V/us\n■摆率> 60V /美国\n■Damping Factor >450\n■阻尼系数> 450\n■Frequency Response (+/-0.1dB)\n■频率响应（+ / - 0.1dB）\n20Hz+20KHz\n20Hz 20kHz +\n■THD (Rated power@ 8 Ohm, 1KHz) <0.01%\n■THD（额定电源8欧姆，1kHz）＜0.01%\n■LMD(Rated power@ 8 Ohm) <0.01%\n■LMD（额定电源8欧姆）＜0.01%\n■Input Sensitivity 0.775V,1.0V,1.55V\n■输入灵敏度0.775V，1.0V 1.55V\n■Input Impedance 10K Ohm Unbalanced;\n■10K欧姆不平衡输入阻抗；\n20K Ohm Balanced\n20K欧姆平衡\n■LPF 20Hz-180Hz Valid\n■LPF 20hz-180hz有效\n■HPF 130Hz-20KHz Valid\n■HPF 130hz-20khz有效\n■Input CMRR <-75dB\n■输入共模抑制比< 75dB\n■Cross Talk <-70dB\n■相声＜70分贝\n■Main Power Supply 220V 50/60Hz,\n■主电源220V 50或60Hz，\nFuse:T10A\n保险丝：T10A\n■Protection Short Circuit, Overload,\n■保护短路，过载，\nOvervoltage, Overheat\n过压，过热\n■Size W*D*H(cm) 48.3*49*88\n■大小W * D * H（48.3×49×88厘米）\n■N.W. 17 kg\n■净重17公斤\n■Unit Piece\n■单元块\n\n","中国","台",4]
[7,"低音功放","YY audio UA1600","■模型pro-800\n■Channel 2\n■2频道\n■8Ω Stereo Power 800W\n■8Ω立体声功率800\n■4Ω Stereo Power 1100W\n■4Ω立体声功率1100\n■2Ω Stereo Power 1300W\n■2Ω立体声功率1300\n■8Ω Bridged Power 2000W\n■8Ω桥接功率2000\n■4Ω Bridged Power 2200W\n■4Ω桥接功率2200\n■Signal to Noise >105dB\n■信号噪声> 105dB\n■Slew Rate >80V/us\n■摆率> 80V /美国\n■Damping Factor >600\n■阻尼系数> 600\n■Frequency Response (+/-0.1dB)\n■频率响应（+ / - 0.1dB）20Hz+20KHz20Hz 20kHz +\n■THD (Rated power@ 8 Ohm, 1KHz) <0.01%\n■THD（额定电源8欧姆，1kHz）＜0.01%\n■LMD(Rated power@ 8 Ohm) <0.01%\n■LMD（额定电源8欧姆）＜0.01%\n■Input Sensitivity 0.775V,1.0V,1.55V\n■输入灵敏度0.775V，1.0V 1.55V\n■Input Impedance 10K Ohm Unbalanced\n■10K欧姆不平衡输入阻抗20K Ohm Balanced20K欧姆平衡\n■LPF 20Hz-180Hz Valid\n■LPF 20hz-180hz有效\n■HPF 130Hz-20KHz Valid\n■HPF 130hz-20khz有效\n■Input CMRR <-75dB\n■输入共模抑制比< 75dB\n■Cross Talk <-70dB\n■相声＜70分贝\n■Main Power Supply 220V 50/60Hz,\n■主电源220V 50或60Hz，Fuse:T10A保险丝：T10A\n■Protection Short Circuit, Overload,\n■保护短路，过载，\nOvervoltage, Overheat过压，过热\n■Size W*D*H(cm) 48.3*49*88\n■大小W * D * H（48.3×49×88厘米）\n■N.W. 27 kg\n■净重27公斤\n■Unit Piece\n■单元块\n\n","中国","台",1]
[8,"数字音频处理器","YY audio KA500","超低音输出具有低切、高切、独立音量控制、自动增益控制等处理模块 *24-bit、48kHz采样率、∑-△ AD/DA转换、32位DSP芯片处理","中国","台",1]
[9,"效果器","BS240","1.2x31段，1/3倍频程；\n2.采用恒定Q值控制滤波器，增益/衰减值可以+/-12dB与+/-6dB之间选择\n3.设有低频切除开关，且其频率可调，消除低频噪声，保护低音喇叭不会过载而烧坏；\n4.采用国外优质芯片，使整机失真小，噪音低，性能更稳定；\n5.直通开光，方便用户与整个系统配合使用；\n6.标准TRS与XLR端，伺候平衡输入输出；\n7.进口20行程推子电位器，手感好，频点控制更准确；\n8.频率响应：20Hz-20KHz，+0/0.5dB\n9.恒定Q值增益衰减：±12dB\n10.工作电平：-10dBu~+4dBu\n11.输入阻抗：40KΩ（不平衡），20KΩ(平衡）","中国","台",1]
[10,"无线手持话筒","YY audio BT-65","接收模式：石英镇定；灵敏度：4uV(up 45 db SINAD/at 15khz deviation)；镜频抑制：>80db；音频输出：不平衡Hio-300mV/10K Mixer, Hio-250mV/10k；供电方式：直流16-20V 250MA输入","中国","套",2]
[11,"16路调音台","YAMAHA  MG166C","设备类型：调音台 纠错 \n规格简述：16个输入通道,10个话筒输入,4组立体声线路输入,1-8通道设三段式中段扫频均衡,9/10-15/16通道设三段式均衡器,前6个话筒通道内置压缩器,所有通道均有高通滤波器,内置SPX数字效果器 纠错\n \n","日本","台",1]
[12,"打碟机","PIONEER  CDJ350S","单CD打碟机","日本","台",1]
[13,"电源时序器","NPW80时序电源","8路时序电源（每通道提供高达10安培电源）\n控制电路采用高可靠性和数字化设计，高电流继电器的输出级和低功耗\n1U和标准万用AC电源插座，可以非常方便使用\n具有开关机锁并配备用户钥匙，管理方便\n面板具有紧急关闭开关，安全方便","中国","台",2]
[14,"合计",{"$nulls":6},0]
["二、音源及点歌服务"]
[1,"单机版点歌机（50000首高清）","歌魔","音视频输出：实现点歌台、电视显示端双向高清（点歌台720P，电视机1080P），高保真SPDIF数字音频输出.全高清DVD原版版权曲库.完美呈现高清画质、炫目3D动感界面，挑战消费者视觉极限。周边配套：支持鼠标、触摸屏、掌中宝、平板电脑、智能手机等多种设备无线点歌；内置50000余首正版高清歌曲。VOD客户端：支持手写、划屏、笔画、拼音、等所有点歌方式。触摸屏：19寸豪华时尚三星LED红外触摸一体机（横屏）","中国","套",1]
[2,"合计",{"$nulls":6},0]
["三、舞台灯光部分"]
[1,"模拟灯控台","DMX192","*192个标准DMX512控制通道\n*可控制12台灯，每台设备多达16个DMX控制通道\n*30个BANK ，8个场景，共有240个场景\n*6个程序，共240个场景\n*4字节数码管显示\n*所有通道可自由配置\n*8个通道推子，可翻页\n*有极性选择开关","中国",1,"台"]
[2,"LED变色灯","LED3W54颗全彩帕灯（防水）","详细说明 \n电压AC:90V-240V/50-60Hz 灯泡:LED 3W一粒 (R,G,B，三合一灯珠)\n\n162WLED铸铝帕灯王 \n防护等级：IP67。\n内置程序自动运行，可联机同步运行 \n标准DMX 512控制器控制，8个通道 \n使用54颗（红12绿蓝白各14颗），每颗3W大功率高亮度LED，亮度高而功耗低，颜色鲜艳  \n铸铝外壳，防水设计，散热效果优良 \n可用于户外使用。严禁直接放于水中  \n电压: 100 - 240V DC \n产品尺寸：290X280X350MM \n包装尺寸：350X350X400MM ","中国",24,"只"]
[3,"LED水晶球","kelek",null,"中国",6,"只"]
[4,"效果烟机","DJPOWER.C-1500","功率1500W，可调输出量。","中国",1,"台"]
[5,"重烟油","DJPOWER","5L","中国",5,"支"]
[6,"中型泡泡机",null,null,"中国",1,"台"]
[7,"泡泡油",null,null,"中国",5,"支"]
[8,"数字频闪灯","RUIXIN.RX-033","1250w灯管，宽光光路，适用于舞台背景的上下光路","中国",4,"台"]
[9,"大玻璃球","24寸",null,"中国",1,"支"]
[10,"小玻璃球","12寸",null,"中国",8,"台"]
[11,"光束灯","KE-MH200A","产品特性\n•本灯具全采用进口色片和隔热片，色温更加均匀统一，保证灯具打出的色彩更加鲜明绚丽；\n•灯具出货默认为台湾YODN R5 200W\n•线路板坚持自主开发，对电子元器件的选择将进一步考虑匹配问题，而不是一味追求价格昂贵的配件，直插式的芯片将统一改成贴片式，实现XY驱动和模块驱动的分离，使线路板更加稳定可靠。\n产品技术规格\n•输入电压：AC100~240V±10%，50/60Hz\n•功率：200W\n•光源：YODN MSD200 5R （可选OSRAM SIRIUS HRI 180W）\n•色温：8000K，光通量7950lm（6m距离），光照度58760lx（20m距离）\n•镇流器：电子镇流器 \n•平均寿命：2000hrs\n•颜色盘：14种颜色+白光，正反双向旋转\n•图案盘：1个图案盘，带17个固定图案+白光，正反双向旋转\n•棱镜：旋转八棱镜，正反双向旋转，效果移动，雾化功能\n•镜头：3片透镜式高品质透镜组\n•雾化效果：0~100%可调雾化的光斑角度\n•光圈：七级光束调节\n•调焦：线性调焦\n•调光/频闪：0~100%线性调光和双片频闪，调速（0.5~14秒）\n•水平扫描：540度，解析度8Bit/16Bit 自动校正\n•垂直扫描：250度，解析度8Bit/16Bit 自动校正\n•光束角度：平行光束角：0~3.8°\n•控制方式：国际标准DMX512 \n•DMX通道：20通道\n•其它功能：机械闭光时光源功率自动减半\n•防护等级：IP20\n•外形尺寸：345mm（臂宽）*475mm（总高）*405（底宽）mm","中国",8,"只"]
[12,"1200W电脑追光灯一体",null,"光    源：HMI 1200W 气体放电泡\n电    源：AC220V±5% 50-60Hz\n功    率：1500W\n功能特点：光圈可调，大小 焦距可调 ，可随意控制\n颜色效果：4种颜色+白光，和彩虹效果功能\n频闪功能：双片式每秒1-10次可变速频闪。","中国",1,"台"]
[13,"合计",{"$nulls":6},0]
["四、设备辅助材料"]
[1,"机柜",null,null,"中国",1,"台"]
[2,"音箱线",null,null,"中国",3,"卷"]
[3,"音频线",null,null,"中国",4,"卷"]
[4,"电源线(强电)",null,null,"中国",2,"卷"]
[5,"大灯钩",null,null,"中国",20,"条"]
[6,"小灯钩",null,null,"中国",24,"条"]
[7,"保险绳",null,null,"中国",1,"批"]
[8,"管材",null,null,"中国",1,"批"]
[9,"接插件、音箱吊架、专用插座、专用数据插座等",null,null,"中国",1,"批"]
[10,"舞台桁架",{"$nulls":6},"自备"]
[11,"合计",{"$nulls":6},0]
["五、设备总计",{"$nulls":7},0]