{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["EV TX系列方案"],"not_rendered":{"images":12},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"EV TX系列方案","index":0,"n_rows":21,"n_cols":12,"rows_kept":21,"merged":[[0,0,0,11],[2,0,2,11],[20,1,20,7]],"flags":["formulas_cached_only"]}
["大连酒吧EV TX系列方案"]
["序号","设备名称","品牌","型号","技术参数","国别","单位","数量","单价","小计","类似图样","备注"]
["扩声设备"]
[1,"15寸主音箱","EV","TX1152","12寸轻便多功能音箱                                                                                    频率响应（-3dB）： 58Hz ~ 15kHz\n灵敏度： 97dB\n最大声压级：131dB\n系统功率：600/1200/2400W\n低频功率：500/1000/2000W\n高频功率：40/80/160W\n阻抗：8Ω（8Ω/8Ω）\n辐射角度（H×V）： 90 º×50 º","美国","只",2]
[2,"主功放","YYAUDIO","Q99","1250W 900W 550W\n额定输出功率（20Hz~20kHz，THD<0.1%）2Ω 4Ω 8Ω： -- 800W 400W\n最大单通道输出功率（动态余量，IHF-A）2Ω 4Ω 8Ω： 2500W 1400W 700W\n最大单通道输出功率（连续，1kHz）2Ω 4Ω 8Ω： 1700W 1100W 630W\n最大桥式输出功率（1kHz，THD=1%）2Ω 4Ω 8Ω： -- 2800W 1800W\n转换速率： 27V/µs\n输入灵敏度（额定功率@8Ω，1KHz）： +5.1dBu\n最大输入电平： +21dBu（8.69Vrms）\n电压增益（1KHz）： 32dB\n信噪比（A计权）： >107dB\n输入阻抗（电子平衡）： 20kΩ\n阻尼系数（1KHz）： >300\n频率响应（1kHz）： 10Hz ~ 40kHz（±1dB）\n总谐波失真（额定输出功率）： <0.03%\n体积（高×宽×深）： 88.4×483×421.5mm\n净重： 16.3kg","美国","台",1]
[3,"返听音箱","EV","TX1122FM","单12寸返听音箱\n频响范围：（-3dB）70Hz～20kHz\n灵敏度 ：99dB\n最大声压级 ：132dB\n额定功率： 500W/8Ω\n覆盖角度 ：H×V：90°×50°","美国","只",2]
[4,"返听功放","YYAUDIO","Q99","1250W 900W 550W\n额定输出功率（20Hz~20kHz，THD<0.1%）2Ω 4Ω 8Ω： -- 800W 400W\n最大单通道输出功率（动态余量，IHF-A）2Ω 4Ω 8Ω： 2500W 1400W 700W\n最大单通道输出功率（连续，1kHz）2Ω 4Ω 8Ω： 1700W 1100W 630W\n最大桥式输出功率（1kHz，THD=1%）2Ω 4Ω 8Ω： -- 2800W 1800W\n转换速率： 27V/µs\n输入灵敏度（额定功率@8Ω，1KHz）： +5.1dBu\n最大输入电平： +21dBu（8.69Vrms）\n电压增益（1KHz）： 32dB\n信噪比（A计权）： >107dB\n输入阻抗（电子平衡）： 20kΩ\n阻尼系数（1KHz）： >300\n频率响应（1kHz）： 10Hz ~ 40kHz（±1dB）\n总谐波失真（额定输出功率）： <0.03%\n体积（高×宽×深）： 88.4×483×421.5mm\n净重： 16.3kg","美国","台",1]
[5,"二楼环绕音响","EV","TX1122","单12寸返听音箱\n频响范围：（-3dB）70Hz～20kHz\n灵敏度 ：99dB\n最大声压级 ：132dB\n额定功率： 500W/8Ω\n覆盖角度 ：H×V：90°×50°","美国","只",2]
[6,"返听功放","YYAUDIO","Q99","1250W 900W 550W\n额定输出功率（20Hz~20kHz，THD<0.1%）2Ω 4Ω 8Ω： -- 800W 400W\n最大单通道输出功率（动态余量，IHF-A）2Ω 4Ω 8Ω： 2500W 1400W 700W\n最大单通道输出功率（连续，1kHz）2Ω 4Ω 8Ω： 1700W 1100W 630W\n最大桥式输出功率（1kHz，THD=1%）2Ω 4Ω 8Ω： -- 2800W 1800W\n转换速率： 27V/µs\n输入灵敏度（额定功率@8Ω，1KHz）： +5.1dBu\n最大输入电平： +21dBu（8.69Vrms）\n电压增益（1KHz）： 32dB\n信噪比（A计权）： >107dB\n输入阻抗（电子平衡）： 20kΩ\n阻尼系数（1KHz）： >300\n频率响应（1kHz）： 10Hz ~ 40kHz（±1dB）\n总谐波失真（额定输出功率）： <0.03%\n体积（高×宽×深）： 88.4×483×421.5mm\n净重： 16.3kg","美国","台",1]
[7,"2进6出处理器","dbx","DriveRack PA+  ","2*6数字控制和信号处理器(可配合RTA-M测试话筒作现场粉红噪声实时频谱分析)","中国","台",1]
[8,"效果器","TC","M.ONE XL","立体声数字混响效果器,双处理器(输入输出采用XLS平衡插头)","丹麦","台",1]
[9,"24路调音台","ALLEN&HEATH","ZED 24","12组单声道,2组立体声,立体声输出，60mm推子，带机架","英国","台",1]
[10,"电源时序器","YY audio","NPW-80","1、工作环境：180V-240V 50/60Hz\n2、电源输入：（3X2.5平方电缆）火线（L）、零线（N）、地线（GND）\n3、输出通道数：后板8路直接接至继电器万用插座输出可控，前板2路万用插座直通输出\n4、整机设备最大输出负载 40A，通道负载输出：单通道最大输出负载 20A\n5、多个同类设备可进行级联\n6、前面板带数码电压显示屏（P-802A），内置40A进口滤波电源","中国","台",1]
[11,"均衡器","dbx","231s","①双路，31段均衡器,带反馈显示； ②频率响应：20Hz—20KHz ±1.5dB； ③总谐波失真：<1%，信噪比：≥98 Db","美国","台",1]
[12,"前级处理器","YYaudio","KA500","音乐\n1. 音乐参量均衡:7段\n2. 音乐到主输出高通滤波器：12dB/24dB(0Hz - 303Hz)\n麦克风\n1. 有四种麦克风FBE模式：OFF 1 2 3\n2. 有麦克风压限功能\n3. 15段麦克风参量均衡\n效果\n回声：\n1. 回声低通滤波器：5.99Hz - 20.6KHz\n2. 回声高通滤波器： 0Hz - 1000Hz\n3. 回声参量均衡：3段\n4. 回声电平：0～100% \n5. 回声直达声电平： 0～100%\n6. 回声预延时：0～500ms \n7. 回声右通道预延时：0～±50% , （相对左声道）\n8. 回声总预延时： 0～500ms\n9. 回声右通道延时：0～50% , （相对左声道回声延时时间）\n10. 回声重复： 0～90%\n混响\n1. 混响低通滤波器可调范围：5.99Hz - 20.6KHz\n2. 混响高通滤波器可调范围：0Hz - 1000Hz\n3. 混响电平可调范围：0～100%\n4. 混响直达声可调范围：0～100% \n5. 回声预延时可调范围：0～200ms\n6. 混响时间可调范围：0～3000ms\n主输出（工作模式：唱歌/热舞 （自动/手动），包含除压限、延时、静音外的所有参数）\n1. 音乐电平： 0～200%\n2. 直达声电平： 0～200%\n3. 回声电平：0～200%\n4. 混响电平：0～200%\n5. 5段音乐参量均衡\n6. 压缩限幅器\n7. 左通道延时：0～50ms\n8. 右通道延时：0～50ms\n9. 左通道静音功能\n10. 右通道静音功能\n中置输出（工作模式：唱歌/热舞（自动/手动），包含除压限、延时、静音外的所有参数）\n1. 音乐电平：0～200%\n2. 直达声电平：0～200%\n3. 回声电平：0～200%\n4. 混响电平：0～200%\n5. 高通滤波器：0Hz - 303Hz\n6. 3段参量均衡\n7. 压缩限幅器\n8. 延时：0～50ms \n9. 静音功能\n超低音输出（工作模式：唱歌/热舞 与 （自动/手动），包含除压限、延时、静音外的所有参数）\n1. 音乐电平：0～400%\n2. MIC直达声电平：0～200%\n3. 高通滤波器：12dB,Q 0.4 ～ 1.5,/Bessel 24dB/Butterworth 24dB/Link Riley 24dB/USER 12dB/USER 24dB (0Hz - 303Hz)\n4. 低通滤波器：12dB,Q 0.4 ～ 1.5,/Bessel 24dB/Butterworth 24dB/Link Riley 24dB/USER 12dB/USER 24dB (0Hz - 303Hz)\n5. 3段参量均衡 \n6. 压缩限幅器\n7. 延时：0～50ms\n8. 静音功能\n系统\n1. 两个音乐输入端口：1/2\n2. 音乐输入增益：0dB/3dB/6dB (用户模式不可调节)\n3．键盘锁密码与系统模式切密码","中国","台",1,{"$nulls":3},"二楼单独播放电影用"]
[13,"落地话筒支架",{"$nulls":3},"中国","支",4]
[14,"航空机柜",null,null,"18U带支撑","中国","台",1]
[15,"主线材","高强信",null,"2.0平方","中国","卷",3]
[16,"接插件",{"$nulls":3},"中国","批",1]
[17,"线管",{"$nulls":6},0,0,null,"自备"]
[18,"合计",{"$nulls":7},0]