{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["EV TX系列小型学校剧场音响"],"not_rendered":{"defined_names":2},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"EV TX系列小型学校剧场音响","index":0,"n_rows":26,"n_cols":10,"rows_kept":26,"merged":[[0,0,0,9],[25,7,25,8]],"flags":["formulas_cached_only"]}
["EV TX系列小型学校剧场音响"]
["序号","设备材料名称","品牌","型号","主要技术参数","数量","单位","单价","小计","品牌注册地"]
["A1 扩声系统"]
["A1.1"," 调音台及录音系统"]
[1,"32路数字调音台","Presonus","Studiolive24.4.2AI","1、24路输入，2路AUX立体声输入 4路编组输出(带最多500ms延时功能)，2路总输出，10路AUX 输出,主、编组、AUX母线可用GEQ\n2、内部处理是全数字方式的，每路输入具有独立的四段参量均衡、压限器、噪声门、高通滤波等\n3、输出部分带两路数字效果器、8通道31段图示均衡\n4、出众的音质：Classic A XMAX专利技术的话筒前置放大器，实现更高的更高的“动态余量”和更低的“本底噪声”以及更纯净的音质感受\n5、JetPLL技术：可以快速锁住任何的数字格式，减少数字部分失真\n6、A/D/A转换采用了迄今最优质的转换器，提供了高达118dB的动态范围\n7、可通过后方火线口，实现扩容，最大实现48通道处理。\n8、后方火线口，可与电脑连接，可实时32x24多轨录音以及多轨播放等功能。",1,"台",null,null,"美国"]
["A1.2"," 扬声器系统"]
[1,"主扩全频扬声器","EV","TX2152","高功率15寸轻便多功能音箱\n频率响应（-3dB）： 58Hz ~ 18kHz\n灵敏度： 98dB\n最大声压级： 132dB\n系统功率：600/1200/2400W\n低频功率：500/1000/2000W\n高频功率：40/80/160W\n阻抗：8Ω（8Ω/8Ω）\n辐射角度（H×V）： 90 º×50 º",4,"只",null,null,"英国"]
[2,"主扩扬声器功放","EV","Q1212","最大中频输出功率（1kHz，THD=1%）2Ω 4Ω 8Ω： 1800W 1200W 750W\n额定输出功率（20Hz~20kHz，THD<0.1%）2Ω 4Ω 8Ω： -- 1100W 550W\n最大单通道输出功率（动态余量，IHF-A）2Ω 4Ω 8Ω： 3400W 1800W 950W\n最大单通道输出功率（连续，1kHz）2Ω 4Ω 8Ω： 2400W 1500W 850W\n最大桥式输出功率（1kHz，THD=1%）2Ω 4Ω 8Ω： -- 3600W 2400W\n转换速率： 30V/µs\n输入灵敏度（额定功率@8Ω，1KHz）： +6.6dBu\n最大输入电平： +21dBu（8.69Vrms）\n电压增益（1KHz）： 32dB\n信噪比（A计权）： >110dB\n输入阻抗（电子平衡）： 20kΩ\n阻尼系数（1KHz）： >300\n频率响应（1kHz）： 10Hz ~ 40kHz（±1dB）\n总谐波失真（额定输出功率）： <0.03%\n体积（高×宽×深）： 88.4×483×421.5mm\n净重： 17.7kg",2,"台",null,null,"中国"]
[3,"拉声像全频扬声器","EV","TX1152","12寸轻便多功能音箱                                                                                    频率响应（-3dB）： 58Hz ~ 15kHz\n灵敏度： 97dB\n最大声压级：131dB\n系统功率：600/1200/2400W\n低频功率：500/1000/2000W\n高频功率：40/80/160W\n阻抗：8Ω（8Ω/8Ω）\n辐射角度（H×V）： 90 º×50 º",2,"套",null,null,"美国"]
[4,"拉声像全频扬声器功放","EV","Q99","1250W 900W 550W\n额定输出功率（20Hz~20kHz，THD<0.1%）2Ω 4Ω 8Ω： -- 800W 400W\n最大单通道输出功率（动态余量，IHF-A）2Ω 4Ω 8Ω： 2500W 1400W 700W\n最大单通道输出功率（连续，1kHz）2Ω 4Ω 8Ω： 1700W 1100W 630W\n最大桥式输出功率（1kHz，THD=1%）2Ω 4Ω 8Ω： -- 2800W 1800W\n转换速率： 27V/µs\n输入灵敏度（额定功率@8Ω，1KHz）： +5.1dBu\n最大输入电平： +21dBu（8.69Vrms）\n电压增益（1KHz）： 32dB\n信噪比（A计权）： >107dB\n输入阻抗（电子平衡）： 20kΩ\n阻尼系数（1KHz）： >300\n频率响应（1kHz）： 10Hz ~ 40kHz（±1dB）\n总谐波失真（额定输出功率）： <0.03%\n体积（高×宽×深）： 88.4×483×421.5mm\n净重： 16.3kg",1,"台",null,null,"中国"]
[5,"‘超低频扬声器","EV","TX1181","单18寸超低音音箱\n频响范围 :（-3dB）50Hz～160Hz\n灵敏度: 100dB\n单18寸超低音音箱\n频响范围 :（-3dB）50Hz～160Hz\n灵敏度: 100dB\n最大声压级 :132dB\n额定功率: 500W/8Ω\n覆盖角度 :全指向",2,"只",null,null,"美国"]
[6,"超低频扬声器功放","EV","Q1212","最大中频输出功率（1kHz，THD=1%）2Ω 4Ω 8Ω： 1800W 1200W 750W\n额定输出功率（20Hz~20kHz，THD<0.1%）2Ω 4Ω 8Ω： -- 1100W 550W\n最大单通道输出功率（动态余量，IHF-A）2Ω 4Ω 8Ω： 3400W 1800W 950W\n最大单通道输出功率（连续，1kHz）2Ω 4Ω 8Ω： 2400W 1500W 850W\n最大桥式输出功率（1kHz，THD=1%）2Ω 4Ω 8Ω： -- 3600W 2400W\n转换速率： 30V/µs\n输入灵敏度（额定功率@8Ω，1KHz）： +6.6dBu\n最大输入电平： +21dBu（8.69Vrms）\n电压增益（1KHz）： 32dB\n信噪比（A计权）： >110dB\n输入阻抗（电子平衡）： 20kΩ\n阻尼系数（1KHz）： >300\n频率响应（1kHz）： 10Hz ~ 40kHz（±1dB）\n总谐波失真（额定输出功率）： <0.03%\n体积（高×宽×深）： 88.4×483×421.5mm\n净重： 17.7kg",1,"台",null,null,"中国"]
[7,"舞台固定返送扬声器","EV","TX1122FM","单12寸返听音箱\n频响范围：（-3dB）70Hz～20kHz\n灵敏度 ：99dB\n最大声压级 ：132dB\n额定功率： 500W/8Ω\n覆盖角度 ：H×V：90°×50°",2,"只",null,null,"美国"]
[8,"舞台流动返送扬声器","EV","TX1122FM","单12寸返听音箱\n频响范围：（-3dB）70Hz～20kHz\n灵敏度 ：99dB\n最大声压级 ：132dB\n额定功率： 500W/8Ω\n覆盖角度 ：H×V：90°×50°",2,"只",null,null,"美国"]
[9,"返送扬声器功放","EV","Q99","最大中频输出功率（1kHz，THD=1%）2Ω 4Ω 8Ω： 1250W 900W 550W\n额定输出功率（20Hz~20kHz，THD<0.1%）2Ω 4Ω 8Ω： -- 800W 400W\n最大单通道输出功率（动态余量，IHF-A）2Ω 4Ω 8Ω： 2500W 1400W 700W\n最大单通道输出功率（连续，1kHz）2Ω 4Ω 8Ω： 1700W 1100W 630W\n最大桥式输出功率（1kHz，THD=1%）2Ω 4Ω 8Ω： -- 2800W 1800W\n转换速率： 27V/µs\n输入灵敏度（额定功率@8Ω，1KHz）： +5.1dBu\n最大输入电平： +21dBu（8.69Vrms）\n电压增益（1KHz）： 32dB\n信噪比（A计权）： >107dB\n输入阻抗（电子平衡）： 20kΩ\n阻尼系数（1KHz）： >300\n频率响应（1kHz）： 10Hz ~ 40kHz（±1dB）\n总谐波失真（额定输出功率）： <0.03%\n体积（高×宽×深）： 88.4×483×421.5mm\n净重： 16.3kg",2,"台",null,null,"中国"]
["A1.3","音频处理设备"]
[1,"系统数字音频处理器","EV","DC-ONE","2进6出数字信号处理器\n带有分频、均衡、延时、压缩及限幅的功能\n带AES/EBU 数字音频输入接口\nDSP:48 kHz采样 32-Bit 浮点处理\n频率响应：10 Hz-22 kHz (+/- 0.5 dB)\n动态范围：111 dB \n输入通道:9段PEQ+31段GEQ+Delay\n输出通道:Routing+5段",2,"台",null,null,"中国"]
[3,"数字效果器","TC Electronics","M3000","双引擎处理技术录音室混响处理器，内置500个厂家预置效果，100个用户自订程序；直观的使用者界面，具有即时预设回忆功能；具有三组细致的电影和后期制作预设效果，备有PCMCIA卡槽，用户可储存自己喜爱的预置。\n接口：XLR模拟输入输出接口、 XLR AES/EBU和S/PDIF数字输入输出接口\n采样频率：44.1kHz，48 kHz",1,"台",null,null,"丹麦"]
["A1.5","话筒"]
[1,"动圈话筒","EV","R300-HD-B","R300无线手持系统 B-Band(678MHz-694MHz)",4,"支",null,null,"美国"]
["A1.6","安装辅材",{"$nulls":7},"中国"]
[1,"高杆话筒支架","K&M","21020-300-55","折叠式的支架腿，立杆二节，及单臂，为K&M工厂的经典款。重量3.2kg，高度900-1605mm，臂长840mm。",2,"支",null,null,"德国"]
["A2 线材及接插件"]
[1,"线材、管线及接插件","定制","定制",null,1,"批",null,0,"中国"]
["A5 工程合计"]
[1,"设备总价：",null,null,"www.pro001.com",null,null,"40万"]