{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["YYaudio中小型学校会议室音响"],"not_rendered":{"images":8},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"YYaudio中小型学校会议室音响","index":0,"n_rows":13,"n_cols":12,"rows_kept":13,"merged":[[0,0,0,11],[12,1,12,4]],"flags":["formulas_cached_only"]}
["YYaudio中小型学校会议室音响"]
["序号","设备名称","品牌","型号","技术参数","国别","单位","数量","单价","小计","类似图样","备注"]
[1,"音箱","YYaudio","YA10","频率响应范围：50HZ-18HZ；单元组成：1X12\"(300mm)3\"1X1\"(25mm)1.7；额定功率：300W RMS,1200Wpeak；灵敏度：97db/1watt/1metre；声压级：122db continuous;128db peak;额定阻抗：8 ohms nominal;","中国","只",4]
[2,"功放","YYaudio","UA800","立体声功率:400W,1KHz0.1 THD 4:600W ,桥按功率:   1000W , \n1KHz0.1 THD 4 1200W ,信噪比:105db ,转换率:60V/μS \n ,阻尼系数:450:1 频响:+/-0.1db,20Hz+20KHZ \n","中国","台",2]
[3,"无线手持话筒","YYaudio","BS-T6","接收机 RECEIVER\n接收频率Frequency Ranges：UHF600-900MHz\n频率稳定度Frequency Stability：±0.002%（用优于15ppm石英晶体锁定）\n灵敏度Sensitivity（peak deviation）：10μV\n鄰道幹擾比F/N Ratio：>8odB\n鏡像干擾比P/N Ratio：>80dB\n信噪比S/N Ratio：>90dB\n扩展比Dilation Ratio：1：2\n音频输出AF Output Voltage（at peak deviation 1kHz AF out）：可调0 ~ 300mV\n接收频道Channels：2路 \n输出接口 Output jack：6.3不平衡混合口 \n电源电压Power Supply：DC 13V-500mA(50Hz\n功耗Power Supply：6W\n天线Antenna：外置天线\n动能范围Dynamic frequency range：>100dB\n综合失真T.H.D：<0.5%\n工作温度Temperature Range：-10℃ ~ 50℃\n\n发射机 TRANSMITTER\n发射频率Frequency Ranges： UHF600-900MHz\n频率稳定度Frequency Stability：0.002%（用优于15ppm石英晶体锁定）\n发射功率 RF Power：30mW\n电流损耗 Cuttent Consumption：< 主波40dB\n制式Modulation Mode：调频FM\n调偏度Deviation Range：±20KHz\n压缩比Compress Ratio：2.1\n拾音器Microphone Head：超心型动圈式\n电池Battery Type：两节5号1.5V碱性电池\n天线 Anternna：外置式 Exterior Antenna\n频率响应 Frequency Response：50Hz ~ 15KHz\n有效距离Receiver distance：50米（理想环境下）","中国","套",1]
[4,"无线会议话筒","KDLK","MI-6000","最多可供16个不同频率选择，同时使用8套互不干扰，话筒开启时，音头发光环点亮，话筒设有低电警告指示灯，具有独立的输出和混合输出功能，可接调音台或功率放大器电源供电","中国","套",2]
[5,"反馈抑制器","behringer","FBQ1000 ","高性能双声道反馈驱逐舰和参数均衡器\n自动和“智能”定位和摧毁多达24个频率\n超窄常见疑难题目过滤器非常有效的反馈抑制，同时保持最高质量\n“劳永逸”的默认设置，使直接和超级简单反馈抑制器的性能\n自动连续监测和自动设置过滤器\n单发模式自动检测并抑制反馈滤波器加锁直到您手动复位\n手动模式可以设置多达24个全参数化滤波器的频率，带宽和增益参数\n广泛的实施和用户即时程序预设记忆回忆\n平衡输入和输出servo-balanced'树木和镀金卡侬连接器\n高品质的元件和极其坚固的结构确保长久耐用","德国","台",1]
[6,"调音台","YAMAHA","MG12XU   ","最多6个话筒 / 12 个线路输入 (4 个单声道 + 4 个立体声) / 2 编组母线 + 1 立体声母线 / 2 AUX (包括 FX）。内置高级效果器：SPX，含24组预置效。可以通过Apple iPad Camera Connection Kit / Lightning to USB Camera Adapter (连接适配器)与iPad (2或更高版本) 连接工作","日本","台",1]
[7,"电源时序器","YYaudio","NPW80","8路时序电源（每通道提供高达10安培电源）\n控制电路采用高可靠性和数字化设计，高电流继电器的输出级和低功耗\n1U和标准万用AC电源插座，可以非常方便使用\n具有开关机锁并配备用户钥匙，管理方便\n面板具有紧急关闭开关，安全方便","中国","台",1]
[8,"机柜",null,"12U","简易机柜","中国","只",1]
[9,"线材/辅材"]
[10,"安装调试"]
[11,"总计",{"$nulls":7},40000,"www.pro001.com"]