{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["AV系统集成"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"AV系统集成","index":0,"n_rows":85,"n_cols":9,"rows_kept":85,"merged":[[0,0,0,8],[1,0,1,1]],"flags":["formulas_cached_only"]}
["分项报价表"]
["2段2层宴会厅"]
["项目","品牌","型号","技术参数","原产地","数量","单位","单价　　　　　　","总数"]
["顯示　 DISPLAY"]
["P4LED全彩显示屏","DYNE","P4","可视面积6.5m*4m,发光单元点间距：4mm；单点像素：1R1G1B；灰度等级256级；最佳视角：水平120度、垂直80度；亮度1200cd/m2；刷新频率400Hz；换帧频率60Hz；驱动方式：动态扫描恒流；寿命：10万小时；","中国",56,"㎡"]
["信号发送接收系统","诺瓦",null,null,"中国",56,"㎡"]
["LED屏安装钢结构",null,"定制",null,"中国",56,"㎡"]
["高清投影机","松下","PT-FDZ97C  \n","单片DLP投影机\n亮度：8500流明  \n分辨率：1920*1200 \n对比度：10000:1\n价格135000元","日本",2,"台"]
["高清投影机","松下","PT-FRZ570C","单片DLP激光投影机\n亮度：5400流明\n分辨率：1920*1200\n对比度：20000:1","日本",2,"台"]
["200寸投影幕","美视","SKYSHOW  200“","自带卷扬系统电动幕","加拿大",2,"张"]
["150寸投影幕","美视","150“","太空/幻彩　白塑幕","加拿大",2,"张"]
["投映机电动升降台","力美","B250","符合标准","中国",4,"台"]
["播控主机","联想","杨天","i7、独显","美国",1,"台"]
["视频处理器","迈普视通",null,"DVI、HDMI、VGA、AV多格式多节目源无缝互切","美国",1,"台"]
["配电系统","正泰",null,"国标","中国",1,"批"]
["HDMI高清矩阵切换器","LBC","RUN1616H","16进16出高清混合矩阵","中国",1,"台"]
["HDMI输入卡","LBC","RUN-HDMI04","支持1920*1200以下任意分辨率，最高支持分辨率1080P/60Hz\n4路HDMI高清信号输入，支持HDMI　V1.3标准和HDCP标准","中国",3,"块"]
["HDMI输出卡","LBC","RUN-HDMI04-O","支持1920*1200以下任意分辨率，最高支持分辨率1080P/60Hz\n4路HDMI高清信号输出，支持HDMI　V1.3标准和HDCP标准","中国",2,"块"]
["微型双绞线 HDMI 和音频收发器","LBC","RUN-HD70Tx/RUN-HD70Rx","最大速率：10.2Gbps\n最大时钟：300 MHZ\n范围：2560x1600@60Hz or 4096x2160@30Hz，3840x2160@30 Hz，4K/UHD@60Hz\n格式：RGB和YCbCr数字视频\n标准1：DVI，HDMI 1.4、HDCP 2.2，cea-861e\n数/信号类型：1 DVI-D（or HDMI）\n连接器：2 DVI-I","中国",10,"对"]
["高清摄像头","FIONTU","HD20","信号系统：-1080i/59.94,1080i/50,1080p/29.97,1080p/25,720p/59.94,720p/50,NTSC,PAL\n传感器：1/3英寸，CMOS，\n总像素：220万，有效像素：207万\n高清输出：HDMI BNC 遵循STMPTE 292M标准\n镜头-20×，f4.42mm～88.5mm,F1.8～F2.8\n数字变焦：16×\n最低照度：0.5Lux@（F1.8，AGC ON）\n快门-1s～1/10000s\n信噪比-≥55dB\n水平视场角：55.2°～3.2°\n垂直视场角：42.1°～2.4°\n视频编码标准：H.264/MJPEG/JPEG\n视频编码码率：32Kbps-16Mbps\n存储功能：支持TF卡（32G）","中国",3,"只"]
["DVD 播放机","Pioneer","DV-310","产品类别：DVD播放机 \n视频特性：双制式纯影院逐行扫描（PAL/NTSC）108MHz/12-bit视频数/模转换器，视频调整，放大功能 \n音频特性：96kHz/24-bit\n产品功耗：11W","日本",2,"台"]
["液晶监视器","PHILIPS","24PFF3661","24寸液晶","中国",3,"台"]
["数字硬盘录像机","大华",null,null,"日本",1,"台"]
["AV 影音面板","Leemc",null,null,"中国",4,"个"]
["SUB TOTAL",{"$nulls":7},{"v":0,"d":"￥0"}]
["音頻　AUDIO"]
["领夹无线话筒","AT","ATW-3110/838","UHF分集式领夹无线话筒\nATW-R3100b分集式无线接收机，\nATW-T310b分集式无线发射机，","日本",4,"套"]
["手持无线话筒","AT ","ATW-3141","工作频率：最少频率间隔：25 kHz；调制方法：FM 调频；额定频偏：±35 kHz；","日本",4,"套"]
["无线话筒接收系统","AT ","DA49","带宽：440～900MHz；增益：+6dB；指向范围：椭圆型90度指向性；类型：无源偶极；接口：BNC","日本",2,"台"]
["无线天线","AT ","ATW-A49","带宽：440～900MHz；增益：+6dB；指向范围：椭圆型90度指向性；类型：无源偶极；接口：BNC","日本",2,"支"]
["现场主扩数字调音台","YAMAHA ","TF5","33个马达推子（32通道+1主控）\n48条输入混音通道（40单声道+2立体声+2返送通道）\n20个AUX（8单声道+6立体声）+立体声+子母线\n8个带有Roll-out的DCA编组\n32个模拟XLR/TRS混合麦克风/线路输入+2个模拟RCA立体声线路输入\n16个模拟XLR输出\n34×34 USB2.0数字录音/回放 + 2×2 录音/回放通过USB存储设备\n1个支持NY64-D音频介面卡的扩展槽","日本",1,"台"]
["备用调音台","YAMAHA","MG16UX","小型数字调音台 \n16个推子，5条母线，3段参量均衡，HPF功能，每通道压限，内置数字效果","日本",1,"台"]
["音乐播放计算机","ThinkPad"," T450（20BVA03NCD）","i7-5500U 8G 16GSSD+1TB 1G独显 Win10","中国",1,"台"]
["计算机外置音频接口","RME ","Babyface Pro","计算机外置数字音频接口\n12输入和12输出通道 \n4 x 模拟输入(话筒、线路、乐器)\n4 x 模拟输出 (2 x XLR, 2 x Phones)\n1 x ADAT I/O或1 x SPDIF I/O光纤 \n1 x MIDI I/O\n1 x USB 2.0 (兼容USB 3)","德国",1,"台"]
["数字音频处理器","APEX","Intelli X²48","数字音频处理器，4入8出，192kHz采样率","比利时",2,"台"]
["主扩扬声器","ADAMSON","S10","2分频，线阵列全频扬声器\n频响范围(±3 dB)：60 Hz - 18 kHz\n指向性(-6 dB) H x V：110° x 10°\n最大声压级（SPL）：141.3 dB\n阻抗： LF 8Ω HF 8Ω\n功率 (AES / Peak)：LF 2x 350 / 2x 1400 W\n                   HF 160 / 640 W","加拿大",8,"只"]
["低音扬声器","ADAMSON","S119","低音扬声器\n频响范围(±3 dB)：30 Hz - 80 Hz\n最大声压级（SPL）：138 dB\n阻抗：8Ω\n功率 (AES / Peak)：1200 / 4800 W","加拿大",4,"只"]
["中置音箱","ADAMSON","P12","2分频，全频扬声器\n频响范围(±3 dB)：60 Hz - 18 kHz\n指向性(-6 dB) H x V：60°x 40°\n最大声压级（SPL）：132.5 dB \n阻抗：8 Ω\n功率 (AES / Peak)：610 / 2440 W","加拿大",2,"只"]
["补声音箱","ADAMSON","P15","2分频，全频扬声器\n频响范围(±3 dB)：55 Hz - 18 kHz\n指向性(-6 dB) H x V：60°x 40°\n最大声压级（SPL）：132.5 dB \n阻抗：8 Ω\n功率 (AES / Peak)：610 / 2440 W","加拿大",4,"只"]
["舞台固定返听扬声器","ADAMSON","PC12","2分频，同轴扬声器\n频响范围(±3 dB)：64 Hz - 18 kHz\n指向性(-6 dB) H x V：60°x 40°\n最大声压级（SPL）：133 dB \n阻抗：8 Ω1720 W","葡萄牙",2,"只"]
["舞台流动返听扬声器","ADAMSON","P12","2分频，全频扬声器\n频响范围(±3 dB)：60 Hz - 18 kHz\n指向性(-6 dB) H x V：60°x 40°\n最大声压级（SPL）：132.5 dB \n阻抗：8 Ω\n功率 (AES / Peak)：610 / 2440 W","加拿大",4,"只"]
["主扩声音箱功放","LAB","FP10000Q","4通道功率放大器\n4*(1300W8Ω，2300W4Ω，2500W2Ω)\n高度：2U\n重量：13.5kg","瑞典",2,"只"]
["补声音箱功放","LAB","FP10000Q","4通道功率放大器\n4*(1300W8Ω，2300W4Ω，2500W2Ω)\n高度：2U\n重量：13.5kg","瑞典",1,"只"]
["返听和中置音箱功放","LAB","FP10000Q","4通道功率放大器\n4*(1300W8Ω，2300W4Ω，2500W2Ω)\n高度：2U\n重量：13.5kg","瑞典",2,"只"]
["线阵扬声器专用吊架","ADAMSON","S-Series Support Frame","符合标准","加拿大",2,"套"]
["电动葫芦","movecat ","BGV D8","1T8m","德国",4,"台"]
["葫芦控制器",null,null,"2路","中国",1,"套"]
["音频跳线盘","Switchcraft ","MT48FN","24通路跳线板\n深度：5.3 in\n高度（机架数）：1.75 in (1 Rack Units)\n位置/触点数量：48","美国",2,"只"]
["音频地插盒","定制",null,"定制","中国",4,"只"]
["音箱接线盒","定制",null,"定制","中国",15,"只"]
["音箱支架","SOUNDKING",null,"符合国标","中国",4,"只"]
["立地话筒架","SOUNDKING",null,"符合国标","中国",4,"只"]
["HUB交换器","H3C","S1224","IEEE802.3 10BASE-T以太网\nIEEE802.3u 100BASE-TX快速以太网\nIEEE802.3ab 1000Base-T 千兆以太网\nANSI/IEEE 802.3 NWay自动协商\nIEEE802.3x流控\n连接器类型：RJ-45\n24个10/100/1000M自适应以太网端口\n支持半双工、全双工、自协商工作模式\n支持MDI/MDIX自适应\n交换容量：48Gbps\n转发能力：35.7Mpps","中国",1,"只"]
["SUB TOTAL",{"$nulls":7},{"v":0,"d":"￥0"}]
["舞台灯光　 Lights"]
["LED成像灯","德晟 ","VIKY-200W","灯珠：COB集成，200W白光；\n功率：250W；\n色温：3200K/5600K；\n显色指数：≥85Ra或≥95Ra；\n电子调光：0-100%线性调光；\n出光角度：19°26°36°50°可选；\n防护等级：IP20。","中国",16,"台"]
["LED聚光灯","德晟","EPS-3544","功率165W；灯珠：3W*54PCS(12R+12G+12B+18W);角度：8° 15° 25°45°可选；防护IP67","中国",18,"台"]
["LED摇头染色灯","德晟 ","MS-3108Z4","灯珠：108pcs3wled\n功率：400W；\n色温：3200K/5600K；\n显色指数：≥85Ra或≥95Ra；\n电子调光：0-100%线性调光；\n出光角度：7--50°可选；\n操作模式：DMX模式，主从模式，\nDMX通道：7/9/11/14通道\n重量：9kg\n颜色：RGBW\n防护等级：IP20。","中国",32,"台"]
["多功能光束电脑灯","德晟 ","MH-230","灯珠：philipsMSDplatinum 7R\n功率：400W；\n色温：8000K\n显色指数：≥85Ra或≥95Ra；\n电子调光：0-100%线性调光；\n出光角度：0--4°可选；\n防护等级：IP20。\n漂亮的点阵显示，四个轻触开关。\n颜色盘：一个颜色盘，每个颜色盘由14个色片+白光组成。\n图案轮：17个图案+白光效果\n效果轮：一个可旋转的八棱镜，雾化功能。水平540度，垂直240度旋转，自动拉回。机械频闪和可调速频闪效果。 \nDMX通道：16/20通道","中国",16,"台"]
["追光灯","飞达","PH1200","光源： MSR1200 W/G22  灯泡 \n色温： 5600K \n焦距调节： 9º~ 16º \n尺寸： 1270*240*305 mm/1010*240*305 mm \n重量： 15.5kg/13.5kg (不含灯架和换色器) ","中国",2,"台"]
["烟雾机","DJPOWER","H-6","功率 1500W\n预热时间 4min\n烟量输出 20000cuft/min\n耗油量（min/L） 10min/L\n最大喷射距离 6m","中国",2,"台"]
["泡泡机","DJPOWER","POPO-1000","功率 60W\n泡泡最大高度 4m\n泡泡最远距离 8m\n耗油量 100min/L","中国",2,"台"]
["雪花机","DJPOWER","S-5","功率 300W\n雪花最大高度 5m\n雪花最远距离 7m\n雪花覆盖面积 15㎡（机器放置在地面45°）\n雪花覆盖面积 30㎡（机器吊挂5m高45°）\n噪音 ≥10M，62db\n耗油量 16.7min/L","中国",2,"台"]
["电脑灯光控制台","YUNPENG","Pearl 2010","2048个通道,可控240台独立地址码的电脑灯,内置闪存驱动器可容纳：- 3000个灯库- 100多个演出程序-外置移动储存卡配置时的选灯方法升级,剧场和重放功能图形发生器15个重放键控制450个场景、程序或剧目。","中国",2,"台"]
["DMX512信号放大器",null,null,"8路DMX512信号放大","中国",3,"台"]
["SUB TOTAL",{"$nulls":7},{"v":0,"d":"￥0"}]
["控制／其他　CONTROL/MISC"]
["控制主机及配件","AMX ","NX-4200","超快1600MIPS处理器\n1GB板载RAM\n1M非易失内存\n8GB SDHC闪存\n1RU机箱高度\n2个AXlink接口\n1 10/100 LAN接口\n4 10/100 ICSLan接口，带PoE\n4 PoE接口\n8数字I/O端口\n2个RS232/422/485端口\n6个RS232-只支持RS232\n8路IR/串行输出端口\n8路继电器端口","美国",1,"套"]
["无线触摸屏","APPLE","IPAD ","品牌: Apple/苹果\n屏幕尺寸: 9.7英寸\n存储容量: 32GB\n操作系统: iOS\n内存容量: 2GB","美国",1,"台"]
["无线触摸屏适配套件","AMX ","TPC-IPAD ","只能用于1个IPAD授权许可使用TPControl控制软件来控制AMX中控系统。","美国",1,"套"]
["有线触摸屏","AMX","MSD-701","1.7\" Modero S 系列墙面安装式宽萤幕触摸屏\n2.显示屏类型：TFT 有源矩阵彩色LCD，采用边缘切换（FFS）- 宽视角技术\n3.显示屏尺寸（WH）：7.3\"*4.8\"（186*122 mm），对角线长8.8\"（222 mm）\n4.分辨率：1024x600  宽高比：16:9\n5.亮度：400 cd/m2   对比度： 800:1\n6.颜色深度：16.7M 色   背光：LED\n7.触摸覆盖：电阻式触摸屏\n8.512M内存和4G闪存 。超宽视角视角：上下和左右178度","美国",2,"台"]
["8路强电控制器","synthesize","LC-REL8","6路20A、2路30A常开,可外部手控，RS232接口、高可靠继电器 ","美国",4,"台"]
["红外线发射电缆（两根）","AMX","CC-NIRC","Netlinx红外线发射电缆","中国",1,"套"]
["串口网络扩展器","AMX","EXB-COM2","1.2路串口网络扩展器，PoE供电，通过网口控制。（注：可选）\n2.提供1个RS-232/422/485数据控制端口和1个RS232接口。\n3.前置面板反馈；数据1-2：支持XON/XOFF和CTS/RTS，300-115,200波特率；\n4.状态：(每通道两个LED)绿色LED为数据发送，RTS、黄色LED为数据接收，CTS、绿色ICSLAN状态LED；","美国",1,"台"]
["专业设备柜","TUTOM ","42U","符合国家标准","中国",2,"台"]
["视听控制软件编程","AMX","AMX","定制中控和IPAD编程","美国",1,"套"]
["SUB TOTAL",{"$nulls":7},{"v":0,"d":"￥0"}]
["費用一覽　COST SUMMARY"]
["显示系統　",{"$nulls":7},{"v":0,"d":"￥0"}]
["音頻系統　",{"$nulls":7},{"v":0,"d":"￥0"}]
["灯光系統　",{"$nulls":7},{"v":0,"d":"￥0"}]
["控制系統　",{"$nulls":7},{"v":0,"d":"￥0"}]
["管线材料费"]
[]
[{"$nulls":5},"Total:",null,null,{"v":4200000,"d":"￥4,200,000"}]