{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["YYAUDIO影院系列"],"not_rendered":{"images":10},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"YYAUDIO影院系列","index":0,"n_rows":26,"n_cols":10,"rows_kept":26,"merged":[[0,0,0,9],[2,0,2,9],[11,0,11,7],[12,0,12,9],[17,0,17,7],[18,0,18,9],[24,0,24,7],[25,0,25,7]],"flags":["formulas_cached_only"]}
["YYAUDIO影院系列方案"]
["序号","设备名称","品牌","型号","技术参数","单位","数量","单价","小计","类似图"]
["一、影院扩声设备"]
[1,"影院主音箱","YYAUDIO","YA15","两个15“低频低音\n4倍中频单元6.5”\n两个15“低频低音\n4倍中频单元6.5”\n大幅面3“新钛高频驱动\n频率响应   40Hz-18kHz\n单元组成   1×15\"(385mm)/3\" voice coil LF\n1×1\"(25mm)/1.7\" voice coil HF\n额定功率   400W RMS,1600W peak\n灵敏度   98dB 1watt/1 metre\n声压级   124dB continuous,130dB peak\n额定阻抗   8 ohms nominal\n指向性   80°x 50°\n分频点   2.2kHz passive\n输入方式   2×Speakon NL4\n包装尺寸   560mm×525mm×800mm\n净重   29.4 kg/pc","只",2]
[2,"影院主音箱","YYAUDIO","YA12","频率响应   50Hz-18kHz\n单元组成   1×12\"(300mm)/3\" voice coil LF\n1×1\"(25mm)/1.7\" voice coil HF\n额定功率   300W RMS,1200W peak\n灵敏度   97dB 1watt/1 metre\n声压级   122dB continuous,128 dB peak\n额定阻抗   8 ohms nominal\n指向性   80°x 50°\n分频点   2kHz passive\n输入方式   2×Speakon NL4\n包装尺寸   480mm×465mm×725mm\n净重   20 kg/pc","只",1]
[3,"影院低音音箱","YYAUDIO","YA18B","频率响应   35Hz-150Hz\n单元组成   1×18＂(460mm)/4＂voice coil LF\n额定功率   600W RMS,2400W peak\n灵敏度   100dB 1watt/1 metre\n声压级   128dB continuous,134 dB peak\n额定阻抗   8 ohms nominal\n输入方式   2×Speakon NL4\n包装尺寸   835mm×645mm×750mm\n净重   49.6 kg/pc","只",2]
[4,"影院侧环绕音箱","YYAUDIO","YA10","频率响应   55Hz-20kHz\n单元组成   1×10\"(250mm)/2.5\" voice coil LF\n1×1\"(25mm) /1.4\" voice coil HF\n额定功率   250W RMS,1000W peak\n灵敏度   95dB 1watt/1 metre\n声压级   119dB continuous,125dB peak\n额定阻抗   8 ohms nominal\n指向性   80°x 40°\n分频点   2.6kHz passive\n输入方式   2×Speakon NL4\n包装尺寸   410mm×395mm×600mm\n净重   14.3 kg/pc","只",4]
[5,"影院后环绕音箱","YYAUDIO","YA10","频率响应   55Hz-20kHz\n单元组成   1×10\"(250mm)/2.5\" voice coil LF\n1×1\"(25mm) /1.4\" voice coil HF\n额定功率   250W RMS,1000W peak\n灵敏度   95dB 1watt/1 metre\n声压级   119dB continuous,125dB peak\n额定阻抗   8 ohms nominal\n指向性   80°x 40°\n分频点   2.6kHz passive\n输入方式   2×Speakon NL4\n包装尺寸   410mm×395mm×600mm\n净重   14.3 kg/pc","只",2]
[6,"2通道功放          ","Wharfedale","S-2500","输出功率 立体声：\n  2x770W/8Ω(0.1% THD at 1KHz )\n  2x1250W/4Ω(0.1% THD at 1KHz )\n  桥接：\n  2500W/8Ω(0.1% THD at 1KHz )\nTHD+N <0.03%\n频率响应 20Hz-20KHz在0/-0.5dB\n  10Hz-40KHz在0/-2dB\n静态噪声 -95dB\n电压增益 33dB\n输入灵敏度 +4dBu\n最大输入电平 +22dBu\n输入阻抗 平衡输入20KΩ,不平衡输入10K Ω\n控制\n 低切滤波器：\n50Hz-6dB(-12dB/oct);30Hz-6dB(-12dB/oct)\n信号指示灯： 输入信号为-35dBu\nClip指示灯： 790Wx2/4Ω输出时灯亮\n限幅指示灯： 800Wx2/4Ω输出时灯亮\n放大器保护： 静音功能;直流保护;过载和短路保护;\n温度保护\n放大器类型 H类线性补偿输出放大器\n电源要求 AC220V，50Hz\n尺寸(HxWxD)\n毫米 96mm x 482.6mm x 427mm\n英寸 3.8\"x19\"x16.8\"\n重量\n公斤/千克 17.7kg\n英镑 39Ibs","台",4]
[7,"3D解码器","YYAUDIO","HD-990","音频处理部分\n1. 支持目前最先进的HD音频解码，包括 Dolby TrueHD、Dolby Digital Plus、DTS Master、DTS HI RES等等。\n2. SD音频解码支持：Dolby Digital（EX）、DTS、DTS ES（D6.1、M6.1）、DTS 96/24、可到192K 7.1CH的PCM等。\n3. 拥有完善的矩阵解码功能：Dolby Pro Logic IIx、DTS Neo:6等。\n4. 智能房间声学特性扫描。\n5. 强大的低音管理：前置、中置、环绕、后置、超低音分组独立调节滤波器拐点、斜率，低音增强功能，单、双后置设置等。\n6. 分组的音调、11段参量均衡器EQ调整。\n7. 独特实用的电子分音及双功放分音技术。\n8. 高品质FM收音，采用专业数字收音芯片。\n9. 具备最长999毫秒的唇音同步技术。\n10. 具备蓝牙接收传输技术\n11. 专业级别的7.1声道平衡端子及RCA输出。\n12. S/P DIF数字信号输出2CH PCM.\n13. 2路带隔离的同轴、2个光纤输入。                                                                                      \n\n二． 视频处理部分\n1. HDMI1.4接口输入、输出。\n2. 4路HDMI输入、1路HDMI输出、HDMI快速切换。\n3. HDMI最高支持1080P，YUV、RGB，支持DVI模式，支持HD音频、8CH LPCM。\n4.支持3D视频播放。\n5. 支持HDMI  CEC控制。\n6.支持HDMI  ARC音频回传。\n7. 视频输入/输出支持：HDMI/DVI  480P、576P、720P50、 720P60、1080i50、1080i60、1080P50、1080P60、1080P24","台",1]
[8,"电源时序器","声准","1018B","8路电源时序器","台",2]
["合计",{"$nulls":7},0]
["二、影院视频部分",{"$nulls":7},0]
[1,"高清投影机（2.35比投影）","丽讯","D5380U","支持全格式 3D。\u000b   \n支持2.35:1真影院宽屏。\n丽讯绝尘技术\u000b。    \n5种可选镜头。       \u000b    \n专为融合拼接而设计的多种功能。","台",1]
[2,"透声投影幕",null,"150寸","3.5*1.5米，2.35:1，透声","幅",1]
[3,"投影吊架",{"$nulls":3},"台",1]
[4,"蓝光DVD","OPPO","BDP-103D4K","BDP-103D延续OPPO人性化的设计和丰富的功能；在BDP-103基础上，对视频部分进行升级，同时采用DARBEE影像增强处理器Altera Cyclone IV和Silicon Image视频处理器SiI9616；全面提升图像细节、物体景深和色阶对比度，带来全新视觉体验和极佳的可玩性。","台",1]
["合计",{"$nulls":7},0]
["五、辅材",{"$nulls":7},0]
[1,"壁挂音箱支架",null,null,"定制","只",6]
[2,"音响线","高强信",null,"3平方","米",500]
[3,"管材",{"$nulls":3},"批",1]
[4,"机柜",null,null,"48u","台",1]
[5,"辅材",null,null,"卡农线、接插件、等","批",1]
["合计",{"$nulls":7},0]
["设备总计",{"$nulls":7},170000]