{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["方案"],"not_rendered":{"images":9},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"方案","index":0,"n_rows":10,"n_cols":10,"rows_kept":10,"merged":[[0,0,0,5],[0,6,0,9],[9,0,9,7]],"flags":["formulas_cached_only"]}
[]
["序号","设备名称","品牌","型号","技术参数","单位","数量","单价（元）","小计（元）","类似图"]
[1,"会议主机","SHURE","DIS CCU","1、全数字音频传输，采用超五类线（屏蔽）标准RJ45 接头；\n2、发言单元与主机线缆，单链长度 120 M，增加中继器最长达 420m\n3、单机可为60个会议单元供电，最多可扩展控制250个会议单元；\n4、自带2种语言同声传译功能，口译单元最大数量可达32台；\n5、提供语音激活、一按即讲和人工控制三种模式；\n★6、全数字化，并采用加密技术防止窃听，最多可同时开启8个麦克风；内置基于网络浏览器的控制界面，可通过智能手机，平板电脑或电脑进行访问；音频输出:8路专业卡侬平衡，音频输入:2路专业卡侬平衡，音频输出可编组路由输出，最大音频输入＞+15 dBm\n7、频率响应：65Hz--16KHz（-3dB)；\n8、总谐波失真（1KHz）：＜0.1%；\n9、动态范围：＞80dB；\n10、 信噪比：＞85dB（A)\n★11、具有报警信号输入接口，当公共广播报警系统启动时，可自动暂停会议，并向与会单元发送报警信息","台",1]
[2,"会议底座","SHURE","DIS DC 5980 P","★1、每个单元可根据需要任意配置为主席单元、代表单元或译员单元 三种权限；内置耳机插孔带音量控制，并可从二个译员通道中选择所监听翻译语种；\n2、内置扬声器，扬声器频率响应：150Hz--15KHz（-3dB)；\n3、可更换的按钮覆盖层，轻触式设计\n4、2个翻译通道","个",20]
[3,"嵌入式基础会议单元","SHURE","DIS DC 5900 F","• 可根据需要配置为主席单元或代表单元；\n• 可根据需要响应按钮条，并确定用户可以使用哪些功能；\n• 内置耳机插孔带音量控制，并可从二个译员通道中选择所监听翻译语种；","个",20]
[4,"嵌入式会议单元面板","SHURE","DIS FP 5921 F","• 可根据需要配置为主席单元或代表单元；\n• 可根据需要选择按钮条，前面板传感器可自动检测相应按钮条，并决定单元的工作方式；\n• 通过适配器可兼容Microflex鹅颈式话筒。","个",20]
[5,"话筒杆","SHURE","DIS GM5923  （40CM）","话筒类型：电容；拾音模式：心形；频率响应：30Hz--18KHz；灵敏度：-52dB(±3dB);最大输入声压级：在3%THD下为110dB spl,1KHz；信噪比：＞60dBA；前后比：＞25dB（1KHz)；长度≦400mm；具有红色LED灯环，指示话筒状态；","支",20]
[6,"数字会议连接线缆-2米","SHURE","DIS EC6001-02","2米串接线","条",19]
[7,"数字会议连接线缆-20米","SHURE","DIS  EC6001-20","20米延长线","条",1]
["合计（含税，不含运费，不含安装调试费）",{"$nulls":7},145322]