{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["VIP包间"],"not_rendered":{"images":9},"read":"whole","date_system":"1900"}

{"sheet":"VIP包间","index":0,"n_rows":16,"n_cols":12,"rows_kept":16,"merged":[[0,0,0,11],[2,0,2,11],[10,1,10,8],[11,0,11,11],[14,1,14,8],[15,0,15,8]]}
["环球音响网 www.pro001.com"]
["序号","设备名称","品牌","型号","技术参数","国别","单位","数量","单价","小计","类似图样","备注"]
["一、扩声系统系统"]
[1,"主扩声音箱","YY audio","YA12","频率响应范围：50HZ-18HZ；单元组成：1X12\"(300mm)3\"1X1\"(25mm)1.7；额定功率：300W RMS,1200Wpeak；灵敏度：97db/1watt/1metre；声压级：122db continuous;128db peak;额定阻抗：8 ohms nominal;","中国","对",1]
[2,"辅音箱","YY audio","YA10","频率响应范围：55HZ-20HZ；单元组成：1X10\"(250mm)2.5\"1x1\"(25mm)；额定功率：250W RMS,1000Wpeak；灵敏度：95db/1watt/1metre；声压级：119db continuous;125db peak;额定阻抗：8 ohms nominal;","中国","对",1]
[3,"低音炮","YY audio","YA118B","频率响应范围：40HZ-150HZ；单元组成：1X18\"(460mm)/4；额定功率：600W RMS,2400Wpeak；灵敏度：100db/1watt/1metre；声压级：128db continuous;134db peak;额定阻抗：8 ohms nominal;","中国","只",2]
[5,"专业功放","YY audio","UA800","立体声功率:400W,1KHz0.1 THD 4:600W ,桥按功率:   1000W , \n1KHz0.1 THD 4 1200W ,信噪比:105db ,转换率:60V/μS \n ,阻尼系数:450:1 频响:+/-0.1db,20Hz+20KHZ ","中国","台",2]
[6,"专业功放","YY audio","UA1600","立体声功率:800W ,1KHz0.1 THD 4:1200W ,桥按功率:2000W, 1KHz0.1 THD 4:2400W ,信噪比:106db,转换率:80V/μS,阻尼系数: 550:1,频响:+/-0.1db,20Hz+20KHZ \n","中国","台",1]
[7,"数字音频处理器","YYAUDIO","KA500","超低音输出具有低切、高切、独立音量控制、自动增益控制等处理模块 *24-bit、48kHz采样率、∑-△ AD/DA转换、32位DSP芯片处理","中国","台",1]
[8,"无线麦克风","YYAUDIO","BS-T6","工作频率：690-740、740-800、800-850MHz；调制方式：宽带FM；信道数目：200；信道间隔：250KHz；频率稳定度：±0.005%；动态范围：100dB；最大偏移：±45KHz；音频频率响应：80Hz-18KHz(±3dB)；综合信躁比：>105dB；综合失真：≤0.5%；工作距离：约100-300m(在没有干扰的情况下)；工作环境温度：-10℃--+50℃\n\n","中国","套",2]
[10,"总计",{"$nulls":7},{"$f":"SUM(J4:J10)","v":0}]
["二、灯光系统"]
[1,"激光灯","红绿KTV之王","T-869","电源：AC96~240V, 50/60HZ, 10W                                                                                                                    激光功率：50mW 532nm 绿激光器\n                     120mW 650nm  红激光器 \n模式:：自走，声控                                                                                                                                      演示效果：激光效果机之王，四马达多图案红绿激光花束。红绿萤火虫+泡泡+60种图案变化，可以红绿黄三色交替，2012年最畅销产品之一","中国","台",1]
[2,"频闪灯","LED三色频闪","VS-39","电压；AC110V-230V\n功率；15W\n频率；50-60HZ\n光源：LED灯珠*112颗\n功能：三色声控频闪/自走/频闪，声控可自调。\n适用场合：舞厅、酒吧、KTV包房","中国","台",2]
[3,"总计",{"$nulls":7},{"$f":"SUM(J13:J14)","v":0}]
["所有总计",{"$nulls":8},{"$f":"J15+J11","v":0}]