{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["雷石点歌系统"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"雷石点歌系统","index":0,"n_rows":78,"n_cols":8,"rows_kept":78,"merged":[[0,0,0,7],[1,0,1,7],[3,0,3,7],[14,0,14,5],[15,0,15,7],[16,3,19,3],[16,4,19,4],[16,5,19,5],[16,6,19,6],[20,0,20,5],[21,0,21,7],[23,0,23,7],[31,0,31,5],[32,0,32,7],[33,0,37,0],[33,1,37,1],[33,3,37,3],[33,4,37,4],[33,5,37,5],[33,6,37,6],[38,0,38,5],[39,0,39,7],[41,0,41,7],[46,0,46,5],[47,0,47,7],[48,3,67,3],[48,4,67,4],[48,5,67,5],[48,6,67,6],[68,0,68,5],[69,0,69,7],[70,1,70,5],[71,0,76,0],[71,1,71,5],[72,1,72,5],[73,1,73,5],[74,1,74,5],[75,1,75,5],[76,1,76,5],[77,1,77,5]],"flags":["formulas_cached_only"]}
["雷石云端90后互联网点歌系统方案  www.pro001.com 环球音响网"]
["一、机房软硬件设备"]
["序号","设 备 名 称","简介","数量","单位","单价\n（人民币）","总价","备注"]
["1.1 机房硬件设备"]
[1,"雷石云主视频服务器","雷石专业云端下载视频服务器8000G型；\n4000G*2块存储(采用4000G高缓存SATA)硬盘/支持云端自动下载歌曲；",2,"台"]
[2,"雷石云从视频服务器","雷石专业云端下载视频服务器32000G型；\n4000G*8块存储(采用4000G高缓存SATA)硬盘/支持云端自动下载歌曲；",1,"台"]
[3,"雷石数据库服务器","雷石保护神数据库服务器，用于保存营业数据",1,"台"]
[4,"云端曲库下载服务器","用于网上下载歌曲，每月3000首HD歌曲自动更新",1,"台"]
[5,"中转服务器","用于内外网中转，不被病毒攻击",1,"台"]
[6,"显示器","19寸液晶/服务器使用",1,"台"]
[7,"主数据交换机","TP-Link 24口全千兆",3,"台"]
[8,"90后云服务推送","30元*31房间*12个月",1,"套"]
[9,"中转路由器","华为",1,"台"]
[10,"KVM 切换器","迈拓",1,"台"]
["小计",{"$nulls":5},{"v":0,"d":"￥0"}]
["1.2机房服务器端软件"]
[1,"云端曲库","云端歌曲库，加歌、替换歌曲，删歌、加电影等；同时还能够导出、导入排行榜方便歌曲管理；\n对系统中所有歌曲处理，达到音量统一均衡，避免歌曲音量大小不一。",1,"套"]
[2,"控制中心","机顶盒采用集中管理、设置、维护、远程开关机；\n设置每个房台的皮肤、公播歌曲、广告信息；发送总台通知、祝福信息、火警信息"]
[3,"火灾报警","火警提示和逃生图：接到总台火警通知后，自动显示该包厢对应的逃生路线图或火警声音。"]
[4,"热迁移冗余备份","多台KTV服务器中，任意一台出现故障停机时，所有包厢会自动点播其它服务器上的歌曲，无需人工干预，营业场所可以不中断运营。\n服务器冗余备份，实现热迁移时对包厢营业没有任何影响。"]
["小计",{"$nulls":5},{"v":0,"d":"￥0.00"}]
["二、包房软硬件设备"]
["序号","设 备 名 称","性能描述","数量",null,"单价","总价","备注"]
["2.1 包房硬件设备"]
[1,"雷石惊艳6000版机顶盒(通过3C认证)","专业的DVD解压芯片，画质流畅无间断,采用嵌入式LINUX技术，除去易坏的电脑硬盘，开关机次数再多也不会损坏，系统稳定.支持双屏切换、支持触摸屏手写、支持双机点歌、支持歌词点歌等最新功能，绿色、节能、低功耗工作",31,"台"]
[2,"19寸点歌屏（A+无亮点）","触摸屏界面可实现与电视界面双屏切换,表面为钢琴烤漆，做工精良，红外屏则具有防水功能，含支架",31,"套"]
[3,"中控盒","既可以将墙板、呼叫铃的信息传递给机顶盒，也可让软件直接控制功放，来调节音量、音调、音效",31,"台"]
[4,"8路灯控盒","用于控制房间灯光",31,"台"]
[5,"门牌灯","定制房间号的门头灯",31,"个"]
[6,"复位开关","用于关闭呼叫",31,"块"]
[7,"小墙板","用于墙面点歌对快速控制",31,"块"]
["小计",{"$nulls":5},{"v":0,"d":"￥0.00"}]
["2.2包房应用软件"]
[1,"雷石客户端点播软件","KTV包房歌曲、电影点播、酒水点单查询、消费明细",31,"间"]
[null,null,"移动练歌房，微信点歌和订房，微信支付，打车，代驾，订房，电影票"]
[null,null,"QQ，百度，酷我，小米，天天动听，支持所有互联网音乐排行榜歌曲同步"]
[null,null,"最美和声，谁是打擂主，中国好声音，我是歌手，快男快女，等选秀节目歌曲同步"]
[null,null,"50000首以上歌曲打分，打分没有上限"]
["小计",{"$nulls":5},{"v":0,"d":"￥0.00"}]
["三、后台管理软硬件"]
["序号","设 备 名 称","性能描述","数量",null,"单价","总价","备注"]
["3.1管理终端设备"]
[1,"雷石收银电脑","前台开关房台收银结帐，打印帐单；\n含19寸液晶显示器",2,"套"]
[2,"收银一体机(超市、厨房、售卖）","房间查询、预订管理；\n含液晶显示器、扫码枪、热敏打印机，钱箱",1,"套"]
[3,"收银打印机","80mm热敏打印机",2,"台"]
[4,"厨房网络打印机","80mm网络热敏打印机",1,"台"]
["小计",{"$nulls":5},{"v":0,"d":"￥0.00"}]
["3.2汇金ERP管理软件"]
[1,"收银管理系统","帐单管理（查账、多付款方式结帐帐单打印、营业报表、收银日记账），全场营业管理",1,"套"]
[2,"咨客管理系统","房台预订管理（房台预订、短信预订、空房、带客、开房、空开房退订及相关报表生成）"]
[3,"出品管理系统","多种出品、分单传菜流程支持，传菜时间效率分析与汇总，货品日盘点和实盘报表统计等"]
[4,"运营管理系统","即时监控营业销售"]
[5,"财务分析系统","财务查询、员工业绩、会员、挂帐、酒水经营、财务数据统计生成报表等"]
[6,"会员管理系统","在经营中对会员管理，实现对会员信息及会员消费的明细的统计"]
[7,"KTV管家系统","总经理控制经营中的应收金额、折扣金额、 签单金额的详细经营情况"]
[8,"佳丽管理系统","方便管理佳丽上下班，考勤，上班频率等"]
[9,"员工考勤系统","员工考勤上下班管理"]
[10,"酒卡管理系统","客户很方便的拿着酒卡来消费，提前绑定客户资源"]
[11,"存酒管理系统","客户喝不完的酒用于存取以便下次支取"]
[12,"送花管理系统","买花送给佳丽，"]
[13,"楼道落单系统","方便服务员快速点餐，开台，退单，换房等"]
[14,"库存管理系统","管理酒水销售出入，盘点剩余多少酒水统计报表"]
[15,"短信管理系统","用于像客户发送本营业场所的最新资讯，活动"]
[16,"泊车管理系统","方便保安停车，找车，管理"]
[17,"IPAD无线点餐","用于无线快速点餐"]
[18,"呼叫响应系统","可以马上呼叫服务员"]
[19,"门牌机管理系统","显示房间号，查询销售情况，点单，广告灯"]
[20,"等......"]
["小计",{"$nulls":5},{"v":0,"d":"￥0.00"}]
["报价合计"]
[null,"名称",{"$nulls":4},"金额"]
[null,"1.机房硬件设备价格",{"$nulls":4},{"v":0,"d":"￥0.00"}]
[null,"2.机房软件系统价格",{"$nulls":4},{"v":0,"d":"￥0.00"}]
[null,"3.包房硬件设备价格",{"$nulls":4},{"v":0,"d":"￥0.00"}]
[null,"4.包房软件系统价格",{"$nulls":4},{"v":0,"d":"￥0.00"}]
[null,"5.后台硬件设备价格",{"$nulls":4},{"v":0,"d":"￥0.00"}]
[null,"6.汇金ERP终端管理软件价格",{"$nulls":4},{"v":0,"d":"￥0.00"}]
[null,"设备=总计",{"$nulls":4},{"v":0,"d":"￥0.00"}]