{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["STARKE"],"not_rendered":{"images":9},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"STARKE","index":0,"n_rows":24,"n_cols":10,"rows_kept":24,"merged":[[0,0,0,9],[2,0,2,9],[10,0,10,7],[11,0,11,9],[15,0,15,7],[16,0,16,9],[22,0,22,7],[23,0,23,7]],"flags":["formulas_cached_only"]}
[" 专业影院设备报价"]
["序号","设备名称","品牌","型号","技术参数","单位","数量","单价","小计","类似图"]
["一、扩声系统"]
[1,"主音箱","STARKE","IC-H3","继承了H7的金圈中高音精华，H3以同级别少有的三分频方式，表达了对极致中高频响应的不懈追求。\n双6.5寸气密式低音，带来精准，低沉而不夸张的低频。","只",2]
[2,"环绕音箱","STARKE","SR3","继承了H7的金圈中高音精华，H3以同级别少有的三分频方式，表达了对极致中高频响应的不懈追求。\n双6.5寸气密式低音，带来精准，低沉而不夸张的低频。","只",2]
[3,"中置音箱","STARKE","IC-H3 CENTER","在很多时候，简单就是美。\n但是简单绝不是简陋和廉价。SR3有一个非常简洁的结构，经典的双极模式。但他采用了和H3一样的金圈高音来增强定位，加强低音的4寸单元来增强环绕氛围。仅仅一对4寸重低音，低频甚至可以下潜至接近70HZ。最重要的是，SR3可以完美的模拟专业影院里的环绕音箱阵列。不是一个发声点，而是用一只音箱产生一面侧面声墙。","只",1]
[4,"低音音箱","Klipsch","SW-310","SW-310 低音炮是同类产品中表现最出色的。采用BASH®数字混合功放和高阻尼、非谐振玻璃纤维编织的驱动和被动式扬声器。\n频响范围:24Hz-120Hz ± 3dB\n最大声压输出:116dB @ 30Hz\n功放:BASH® Digital Hybrid\n功放功率:400W 持续 / 900W 峰值\n驱动组件:10\" (25.4cm) 主动 / 双 10\" 被动","只",1]
[5,"AV功放","YAMAHA","RX-A2040","AVENTAGE 9.2声道内置Wi-Fi网络数码家庭影院功放拥有4K 50/60p支持、高清多媒体接口区域切换功能等特点，采用了高保真设计包括对称功率放大器、高分辨率音频设计和两个高品质ESS数模转换器。支持最新环绕音效格式“杜比全景声” (Dolby Atmos®)","台",1]
[7,"蓝光播放器","OPPO","BDP-103","Marvell Qdeo技术\n视频降噪处理（VNR）\n精准转逐行处理（De-interlacing）\n边缘增强调节（Edge Enhancement）\n将任意视频源上转换为4K（3840 x 2160）分辨率输出\n只需按一下遥控按键，就能将普通的DVD、蓝光和其他视频内容转换为3D画面，带您进入另一个维度。","台",1]
[9,"电源时序器","声准","1018B","8路电源时序器","台",1]
["合计",{"$nulls":7},0]
["二、背景音乐系统"]
[1,"带后盖天花喇叭","KDLK","LS-604H","6W、6.5″单元，ABS塑料,频响110-15KHZ，外观尺寸φ220*110，开孔尺寸φ200","只",12]
[2,"1.5U带MP3/FM广播功率放大器 120W","KDLK","NP-120","内置MP3解码播放器与FM收音机播放器，可自由切换播放模式；支持U盘及SD卡存储歌曲，更换歌曲方便；配带遥控，方便操作；采用先进高效功率放大电路，设有2路话筒输入，3路线路输入，1路辅助输出， 电压输出为70V/100V，定阻输出为4-16Ω，输出功率为120W，输出频响范围为100~16KHz；每路输入音量可独立控制，带有高低音音量调节；话筒1设为最高优先功能，自动抑制其他输入信号；设备设有异常工作保护警告功能，当输入信号过大、负载过重、温度过高、线路短路时，对应的指示灯提示，有极高的可靠性。 1.5U标准机箱设计，铝合金面板，美观实用。箱体尺寸435*66*280mm，电源功耗为204W","台",1]
[3,"播放设备",null,null,"U盘或电脑或dvd","台",1,0,0,"自备"]
["合计",{"$nulls":7},0]
["二、线材辅材"]
[1,"音响线","高强信",null,"2.0平方","米",200]
[2,"接插件",{"$nulls":3},"批",1]
[3,"管材",{"$nulls":3},"批",1]
[4,"音箱吊架",{"$nulls":3},"只",5]
[5,"机柜",null,null,"16U","台",1]
["合计",{"$nulls":7},0]
["总计",{"$nulls":7},0]